METHOD STATEMENT  

FOR TREE PROTECTION 







LOCATION: 








23 Crimsworth Avenue, Chorlton 






1) 






All trees to remain on site to be adequately protected during construction and other 

operations in accordance with BS 5837 : 2012 “Trees in relation to Design, Demolition 

and Construction.”  Protection fencing shall be erected prior to any operations on site, 

and shall be considered sacrosanct.  It shall not be removed or breached during 


operations without prior consultation with an arboricultural specialist and the approval 

of the Local Authority. 



2) 




As large an area around each tree as possible shall be protected.  The minimum distance 

for the erection of protective fencing around each tree is below the outermost limit of 

the branch spread or at a distance equal to half the height of the tree, whichever is the 

further from the tree trunk. 



3) 




Herras Fencing positioned at the outer edge of the Root Protection area, securely 

staked and with RPA warning signs attached, shall be erected in accordance with 2 


above.  Fencing shall be secured on posts at either end and at intervals of not more than 


4.5 meters, in accordance with the distance around each tree specified in 2 above. 



4) 




No activities or materials shall be allowed within the fenced-off area.  Notices should be 

erected on the fencing with such words as “Protected Area – no operations or materials 

within the fenced area.” 
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5) 

If it is essential that protective fencing has to be moved closer to the trunk than the 

distance stipulated in 2 above, for example to allow scaffolding for building works 

beneath the canopy spread of the tree, it should be as far away from the tree as 

possible.  Boarding should protect the ground between this fencing and the building 

(eg. Scaffold boards) in accordance with Figure 6 of BS 5837.  



 A single thickness of boarding laid on the soil surface will provide sufficient protection 

for the pedestrian loads, but more substantial boarding should be left undisturbed and 


should be protected with a porous geotextile fabric.  



 If necessary, sand should be laid on the fabric to level the ground.  When required, the 

building scaffolding should be erected on the boards.  The boarding should be left in 

place until the building works are finished. 



6) 




If tree roots are in evidence beyond the fencing, such fencing should be extended to 


protect the roots.  If this is not practical due to the roots being located where they may 

be liable to damage by vehicles, machinery or operations, advice should be sought from 

an arboricultural specialist.   



7) 




Additional precautions outside the fenced areas should be taken to avoid damage to 

trees in the following ways: 



a) 




Oil, bitumen, cement or other material likely to be injurious to a tree should not be 

stacked or discharged within 10m of a bole, and materials generally should not be 


stacked or discharged within 5m of a bole. 



b)  Concrete mixing should not be carried out within 10m of a tree. 
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c) 

If possible, trees to be conserved should not be used as anchorages for equipment 

used for removing stumps, roots or other trees, or for any other purposes.  When 

this is unavoidable, the trees should be protected in accordance with the 

recommendations of BS 3998. 




d)  Notice boards, telephone cables, or other services should not be attached to any 

part of the tree. 




e)  Care should be exercised when using cranes or similar equipment near the spread of 

the canopy of a tree. 



f) 




It is essential that allowance should be made for the slope of the ground so that 

damaging materials such as concrete washings, mortar or diesel oil cannot run 

towards trees or hedges. 
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