03RD November 2021
 
Building Regulations Specification 
390 Great Western St, Rusholme, Manchester, M14 4HA.

General
Note to contractors: All dimensions must be checked on site prior to any works commencing on site.
All works are to comply with the relevant British Standards / EU requirements, and current Building Regulations.
Local Building Control inspector to be contacted prior to enclosing any detail that may need to be inspected and approved.
Contractor to ensure that any materials / details are within the requirements of the Planning Application Approval and in accordance with any conditions that may be attached (i.e. brick colour or type).
All new lighting points to be fitted with energy saving bulbs.

Foundations
Any existing foundations or lintels that are subjected to additional loading are to be exposed, inspected and approved by Building Control Officer prior to the commencement of any works on site. Where elements are found to be inadequate, then remedial works to be carried out to the approval of the Building Inspector.

New External Walls (Maximum U-Value : 0.28W/m²K)
External brickwork to match existing. 
100mm cavity fully filled with Dritherm 37 or similar.
Blockwork to be Celcon Standard or similar.
Wall ties to be stainless steel type A. Fixed at 900mm horizontal centres and 450mm vertical centres (2.5 per m2). Amount of ties to be increased to 300mm vertically around new openings and at verges.
Brickwork to be toothed in and all cavities to be continuous where new walls abut existing property.

Internal non-loadbearing walls
75mm x 50mm timber studs fully filled with insulation. Noggins at midspan. Plasterboard and skim to both sides.
Openings
All structural beams, fixings and supports to be as per engineers details - a conditional approval is requested for this item.
New steelwork to be supported off concrete padstones.
All new lintels are to be Catnic or similar with a minimum end bearing of 150mm. 
All new steelwork / lintels are to be boarded with 12.5mm plasterboard and skimmed in order to provide a minimum of 30 minutes fire protection.
Cavity trays to be seated directly above external lintels and weep holes to be provided externally.
Thermabate (or similar) cavity closers to be installed to all jambs and cills of new openings (blockwork returns not permitted).


[bookmark: _GoBack]Pitched Roof (Maximum U-Value : 0.16 W/m²K)
Roof tiles to match existing (to be adequate for pitch and no less than 17.5 degrees).  
Breathable felt laid with minimum 150mm lap over diminishing preformed trusses (trusses and bracing to be fixed in accordance with BS5268).
Tile battens to be 25 x 50mm.
Wallplate to be 100mm x 75mm fixed to inner skin of blockwork. 
900mm long m.s. straps to be fixed at 2m centres to rafters, ceiling joists and wallplate.
Insulation to be 300mm glass fibre insulation laid in 150mm layers at right angles. 
Plasterboard and skim to underside of ceiling joists.
150mm Code four lead valleys on 300x25 lay boards. 
UPVC facia board and soffits (colour to match existing).

Windows (Maximum U-Value : 1.6 W/m²K)
All windows to be double glazed k-glass 4-16-4 argon filled.
Toughened glazing to be installed to any windows and doors where the glass is below 800mm from finish floor level, within and adjacent doors.
All windows to be fitted with trickle vents. 
Escape windows to all new first floor bedrooms. Min openable area 0.33m2 with no dimension less than 450mm. (please note: any existing window openings that are to be altered are to made into escape windows).
Cills to windows to be no lower than 800mm or any higher than 1100mm from finish floor level.
All new windows and doors to be in accordance with PAS24:2012.

Electrics
Any new electrics or any alterations to the existing electrical layout are to be carried out by a certified electrician and be a member of an approved body such as NAPIT, Elecsa etc. Certification to be provided upon completion. This certification is to be issued to the relevant Building Control body within 5 working days of completion.

Heating 
Alterations to the existing heating system or the provision of any new heating installation (including flues) to be carried out by a qualified Gas Safe engineer. Certification to be provided within five working days of completion and submitted to the relevant Building Control body.

Fire Protection 
All lintels and beams to have a minimum of 30 minutes fire protection - 12.5mm plasterboard and skim.
Smoke alarms to be fitted within entrance lobby and first floor landing. All alarms to be mains wired, interlinked and provided with battery backup.
Heat detector to be provided within kitchen area.

Below Ground Drainage
Manholes / rodding eyes are to be positioned over any point in which the drain changes direction. 
All new drainage to be laid to falls no less than 1:40 and to be 100mm diameter plastic.
Separate drainage system to be maintained where possible.


Above Ground Drainage 

WHB : 32mm diameter waste pipe, 75mm deep seal anti-syphon trap, connecting into the SVP.
W.C : 110mm diameter waste pipe, 110mm diameter p-trap, connecting into SVP. 25mm diameter overflow pipe to discharge externally.
Shower : 40mm diameter waste pipe, 75mm deep seal anti-syphon trap, connecting into SVP.
All new drainage to connect into existing SVP.
SVP to be 100mm diameter pvc and to extend 900mm above any opening within 3m when discharged externally.

External Drainage
Gutters to be 100mm half round pvc. 
Downspouts to be 65mm pvc.

Background Ventilation
Habitable Room:
Rapid Ventilation to be a minimum of 5% of the floor area within each habitable room.
Background Ventilation 8000mm2.

Kitchen:
Rapid Ventilation to be via opening window.
Background Ventilation 4000mm2

Bathroom:
Background Ventilation 4000mm2.

Mechanical Ventilation

Kitchens - 60 l/s or 30l/s where close to cooker hood.
Bathroom /  WC's - 15 l/s

General Items :

Locations of electrical & heating points to be agreed with client prior to installation.
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