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1.0
INTRODUCTION
1.1
This information is based on ‘The Construction (Design and Management) 




Regulations 2015 and the ‘Construction (Design and Management) Regulations 


2015. Guidance on Regulations “Managing Health & Safety in Construction” as 


published by the Health and Safety Commission. 

By its nature the Pre-Construction Information Package is a live document and the information contained therein cannot be considered as complete until the final construction work is being undertaken.  The document is therefore subject to alteration and or addition throughout the construction period.

1.2
This information has been obtained from various sources including the Client and


Design Team.  Particular key hazards are identified in relation to the type of


construction and materials which may be encountered and site wide matters, later in 


Section 5.

1.3
This information is prepared on the basis that the Principal Contractor has the required 

skills, training and knowledge and where they are an organisation, the organisational 

capability to carry out the work in a way as defined in of the 2015 CDM Regulations.  

The Principal Contractor is deemed to be aware of and must comply with:



The Construction (Design and Management) Regulations 2015



The Health & Safety at Work etc Act 1974, and subsequent amendments



The Management of Health & Safety at Work Regulations 1999 amended 2007

and all other relevant health and safety related legislation current at the time of carrying out these works.

1.4
The Principal Contractor must also plan for co-operation with the Design Team and all 

the construction team members are specifically reminded of their legal responsibilities 

under HASWA 1974 and other Regulations made under that.

1.5
The Principal Contractor is charged with the good management of the project and 


further reference should be made to the following:



HSE "Successful Health and Safety Management" HS(G)65.



"Construction Safety" (2 no. volumes) published by the Building Employers Confederation.



HSE "A Guide to Managing Health and Safety in Construction".



HSE "Designing for Health and Safety in Construction".



C552, Contaminated Land Risk Assessment A Guide to Good Practice, 2001.
HSG168: Fire Safety in Construction

BS 6187:2011: Code of practice for full and partial demolition
1.6
The Designers, through meetings and considering alternatives, have tried to design out 

both construction and residual hazards. Information in this document in Section 5


attempts to identify particular hazards which may still exist and not be obvious to the 


Principal Contractor.  It does not include identification of common construction 


hazards which are self evident and which may reasonably be expected to be familiar 


to a competent Principal Contractor. 


The Package has been prepared with care and attention to the knowledge available at the time.  However, neither the Client nor the Principal Designer can guarantee the sufficiency of the information.
1.7
The Construction Phase Plan for the project is to be prepared by the Principal
Contractor to incorporate this information, as required by Part 3, Regulation 12 of the 2015 CDM Regulations.  This Package has been prepared by Michael Oughton Associates as the Principal Designer and is in accordance with Part 3, Regulation 11 of the 2015 CDM Regulations.  The duties under the “Construction (Design & Management) Regulations 2015 are additional to and do not replace the general and specific duties placed upon Contractors under the Health and Safety at Work etc Act 1974, the Management of Health and Safety at Work Regulations 1999 (amended 2007) or any other statutory provisions relating to their activities.

1.8
The Construction Phase Plan will contain information on health and safety obtained 
from the Client, Designers, Principal Designer, Statutory Undertakers, Principal 
Contractor and Contractors involved in the construction of the project. All parties 
are to take the Plan into account in discharging their duties. The Plan should be kept 
under review throughout the duration of the project and may be modified to reflect 
changing circumstances as the design is developed and the construction work 
progresses.  The plan will be inspected by the Principal Designer who will advise the 
Client on its sufficiency to make a safe and practical start to the works.

1.9
The Principal Contractor is responsible for ensuring that all costs he will incur as a result


of complying with the Construction (Design and Management) Regulations 2015, all 


relevant Health and Safety legislation, and the requirements outlined in this Information 


Pack have been taken into account. The Information Package forms part of the 


Tender Documents and must be priced by the Principal Contractor and, where 


appropriate, costs must be identified against the appropriate Contract Preliminary


items.

1.10
The appointed Principal Contractor shall develop and implement the Construction


Phase Plan and his own outline method statement(s) before the Construction Phase


starts in accordance with the Guidance on Regulations L153 Construction Plan in 


Appendix 3.  During the execution of the works further information may be 




discovered or become available and therefore this will be 
distributed by the 


Principal Designer to the Designers and/or Principal Contractor at any time up to 


Practical Completion. 

1.11
Section 6 of the Package provides a basic outline of the Health and Safety File, but co-

operation is required with the Principal Designer throughout the project to ensure a 


copy of all useful information is saved.

1.12
In accordance with the Regulations, the responsibility for compiling and issuing the 
Health and Safety File rests with the Principal Designer. Designers and contractors 
are required to provide the information for inclusion in the Health and Safety File to 
the Principal Designer as it becomes available and is not to be withheld until the 
project has been completed.

1.13 
The government’s Covid 19 guidelines must be met within the lockdown period the requirements of which are indicated on the attached risk assessment, all activities will be planned to allow distancing and mess & wash facilities

2
DESCRIPTION OF THE PROJECT
2.1
Project description and programme details:
The project comprises a traditional procurement for the construction of a new three storey residential property.

The works comprise the construction of new foundations and floor slab, drainage, manholes and connection to the existing drainage system. New external cavity walls supporting a timber rafter roof with a slated or tiled roof finish. UPVC windows and doors externally.
Intermediate timber floors supported off load bearing walls and a steel framework, timber staircases, load bearing and non-loadbearing internal walls and partitions, doors and frames, decorative joinery, wall, floor & ceiling finishes, fitting out of bathrooms and kitchen, mechanical & electrical installations, internal and external decoration, external works of hard and soft landscaping and fencing works


Key dates planned for start and finish of the construction phase are:


Start on site:
1st December 2021

Duration
30 weeks

Completion:
29th June 2022

The minimum time to be allowed between appointment of the Principal Contactor

and instruction to commence work on site is 2 weeks
2.2 Details of Client, Designers, Principal Designer and other Consultants:

CLIENT  
The Egerton (Property) Partnership Limited
Lancaster House, 

70-76 Blackburn Street, 

Radcliffe, 

Manchester, 

M26 2JW 
Telephone





PRINCIPAL DESIGNER
Michael Oughton Associates
46 Manchester Road






Chorlton







Manchester, 

M21 9PH

Telephone
0161 881 5216
Contact

Mike Oughton

Email

mike.oughton@baqus.co.uk

Mobile

07976 517466

ARCHITECT 

Simon James Arq Limited
1st Floor

120 Grovenor Street
All Saints
Manchester 
M1 7HL
Telephone: 

07787 744715
Contact: 

Simon James
Email:


simon@simonjamesarqltd.com
2.2     Details of Client, Designers, Principal Designer and other Consultants
STRUCTURAL ENGINEER 

STL Projects Limited
1 Barkers Lane
Sale
M33 6RP

Telephone:

 0161 969 3218
Contact: 

Simon Crowe
Email:


info@stlprojectsltd.co.uk
          Health and Safety Executive Local Office 

Health and Safety Executive

Redgrave Court

Merton Road

Bootle

Merseyside, 

L20 7HS

2.3
Whether or not the structure will be used as a workplace (in which case, the 
finished 
design will need to take account of the relevant requirements of the Workplace 
(Health, Safety and Welfare) Regulations 1992):
The building will not be used as a workplace and therefore the WHSW Regulations 1992 will not apply.

2.4
Extent and location of existing records and plans. 

2.4.1 
Existing Health & Safety Files: 


a) There are no existing Health & Safety Files for the site
2.4.2   Consents: 
a) Planning Consent has been granted for the proposed works.

b) Building Regulation Approval is required for the proposed works.

2.4.3    Surveys and Reports: 

a) Asbestos Survey is not required
b) Ground Investigation report has been undertaken.

c) Flood Risk Assessment has not been commissioned

d) Ground Penetrating Radar Survey has not been commissioned

e) Ordinance survey is not required
The existing plans and records for the scheme are as follows:
The records of services running across the site to serve the adjacent building have been included within the attached appendices to this plan, there is evidence of services crossing the site to whole of the existing buildings. However these records are not a definitive record, therefore prior to excavation works, and drainage works commencing, a survey of the site will be carried out with a CAT and Genny to determine the presence and location of buried services local to the buildings. All live services found will be clearly marked by pins, signs, etc. Information on buried services will also be included in the site induction procedure. 
2.5
The Site
The site lies on Crimsworth Avenue and is a prepared site within the grounds of the client’s property. The site has limited access to the work area off Crimsworth Avenue and it is a cul de sac . The adjacent properties are other residential properties.
3.0
CLIENT’S CONSIDERATIONS AND MANAGEMENT REQUIREMENTS

The covid 19 Virus is controlling the type of work and work processes, therefore prior to any work starting on site a full assessment is required to confirm what activities can be carried out in light of the government’s guidelines and the attached risk assessment

3.1
Planning for and managing the construction work, including any health and safety


goals for the project.

The Client’s goal is to construct the project safely and without risk to the health and safety of site operatives, members of the public and occupants of the building. Care is to be taken during the design and construction processes to ensure as far as practicable that the finished building is safe to clean and maintain with the minimum of specialist equipment.  As far as is reasonably practicable the “General Principles of Prevention” will be observed.  These are to be found in Appendix 7 of the Approved Code of Practice “Managing Health and Safety in Construction”.

The Principal Contract should strive to ensure:


a)
all work is to be carried out in a manner that does not unduly endanger the 


health and safety of anyone working on the project or anyone else affected 

by the work activities;


b)
there is to be full compliance with all relevant health and safety legislative
 


requirements and with all the additional instructions identified within this Pack.



Tenderers are to include within their Tender for all duties required as Principal Contractor including the preparation of a Construction Phase Plan and demonstration to the Client of its adequacy prior to commencement of the works on site.



The Principal Contractor will manage safety during the construction works and will develop and maintain the Construction Phase Plan as appropriate.  The Plan must be available on site at all times for reference by those carrying out the works.  The currency and validity of the Plan will be kept under review throughout the works.  The Principal Contractor must state what site arrangements he will have in place for monitoring health and safety standards during the works.



Any client representative (e.g. Safety Officer, Project Manager, Designer, Principal Designer, Clerk of Works, Building Surveyor) will have the right to request safety information and remedial action as necessary.

3.2
Communication and liaison between Client and others.

The Client and Principal Designer will ensure that design meetings will be held to encourage cooperation and for the design team and construction team to work together effectively. The construction meetings will be structured to ensure that there is clarity as to the roles, functions and responsibilities of the project team. The meetings will ensure there is good communication, co-ordination and co-operation between members of the project team.

Designers will be able to confirm that their design & any changes to the design, have taken account of the responsibilities of regulations 11 and 12.

3.2
Communication and liaison between Client and others.

The Design Team have produced a fully designed and coordinated design to ensure that the goal of an accident free project can be planned and managed

Design changes are to be tabled during site meetings and the health & safety, implications are to be discussed with the Principal Designer & Principal Contractor prior to implementation. Any design change which will affect health & safety within the contract period and subsequent use of the buildings are to be fully documented within the Health & Safety File. The Health & Safety Plan will be continually assessed & will be amended to incorporate design & other changes as & when they arise. Copies of the site meeting minutes are to be provided for the Health & Safety File.


The management of health and safety through the works will be the Principal Contractors responsibility, however where issues are external to the site, for example when working adjacent to the shared pavements, he will be expected to liaise with the Client and adjoining building or land owners before works are carried out, providing Method Statements and report updates.

3.3
Welfare provision for workers.


The Covid 19 requirements have made several amendments to what has to be included as part of the site welfare requirements the statement below indicates the minimum requirement and the construction phase plan will have to indicate how safe distancing will be managed and the cleaning regime for common areas including additional hand cleaning points throughout the site.

Reference should be made to Welfare facilities as outlined in the 2015 CDM Regulations, Schedule 2.  
A position for the welfare accommodation has been identified within the existing garden area on the Crimsworth Avenue, elevation, there is opportunity to use the positions in the building as the construction progresses
Given the nature of the site due consideration shall be given when locating temporary accommodation with respect to access by third parties, operatives and site vehicles a position adjacent to the site entrance has been identified for this use. The Principal Contractor shall prepare a layout plan identifying the position & repositioning of all temporary accommodation in the detailed construction phase Health and Safety Plan prior to the commencement of the works on site. Contractors welfare accommodation is to be provided as follows:-  Heated messing accommodation for site personnel with seating and tables, dedicated drying & changing facilities. Fresh water for drinking and facilities for boiling water. Washing facilities, hot and cold running water. Sanitary provisions. The welfare provision is to be fully detailed within the construction phase health & safety plan, including any repositioning. As a minimum standard there must be 1 wash basin to 12 operatives & 1 WC to 20 operatives. HSE information sheet No. 18 (revised) and as outlined in the 2015 CDM Regulations, Schedule 2 which

 provides guidance as to the type & size of welfare provision that is required.

3.4
Security of the site.

The security of the site does raise health & safety issues as the site is surrounded by public pavements on all elevations, therefore adequate security measures will be required to the site, site compound and the work area. These measures are to include adequate fencing, hoarding, signage and entrance security measures

The Principal Contractor shall institute and enforce a signing-in system for all
operatives and visitors to the site. The Principal Contractor shall advise visitors of any hazards on site whether or not in areas to be visited.




The Principal Contractor will be required to prepare a Site Layout Plan, prior to


commencement of work on site, which should include details of temporary security


fencing and other security arrangements.  
3.5
Requirement relating to the health and safety of the client’s employees or customers or those involved in the project such as:

There are no clients operations during this project.

Should any of the Client’s Employees or contractors require entry into the site or building during the construction phase, then arrangements for access etc must be made directly with the Principal Contractor.
3.6
Site transport arrangements or vehicle movement restrictions.

Location and repositioning of locations for storage areas are to be indicated on the layout plan submitted with the construction phase Health and Safety Plan, the management of on-site deliveries are to be detailed within the construction phase health & safety plan. The section of the existing adjacent accommodation land indicated on drawings may be used for storage purposes subject to adequate protection being provided to the surface.
Deliveries to the site externally are to be planned by the Principal Contractor to both limit highway hazards and cause minimum disruption to the adjoining access roads. 

All vehicles should be selected to suit entrance road widths available.  Instructions on the delivery route and agreed restrictions should be sent with all orders.

A banksman should be provided, where necessary, by the Principal Contractor for all vehicles moving within the site boundary.

 The speed of all vehicles is to be controlled to consider presence of public and other vehicles in the entrance zone. 

Working methods adopted shall allow the safe segregation and protection of the public, adjoining building owner’s employees, the Client’s employees (if applicable) and Consultants from other construction activities.
3.7
Client permit-to-work systems.

The principal contractor is to enforce his own permit to work system.
3.8
Fire precautions.



Increased requirement for keeping site clear of debris especially combustible materials as several of the escape exits will be blocked by the construction works as the works proceeds. The provision of a temporary fire alarm & emergency lighting system is to be installed on the site as soon as is practical. Clearly indicate position of fire exits & fire fighting equipment. Prevent fires from occurring, follow clear rules for hot works in particular ensuring fire extinguishers are at hand and the work area is checked at least one hour after completion of the works for smouldering etc., keep a tidy site and remove rubbish promptly & regularly, avoid unnecessary stockpiling of combustible materials limit what is taken onto site to what is needed for a days work, do not burn waste on site, make sure everyone abides by site rules on smoking.

The Principal Contractor is responsible for the fire control and prevention procedures throughout the course of the project.
3.8
 
Fire precautions
The Principal Contractor shall ensure that all equipment, methods, and materials are of a safe nature and he is to take all necessary precautions against fire and that fire escape routes are to be kept clear at all times.

Fire extinguishers in sufficient numbers and types are to be readily available at all times. These shall be both provided and located around the building as the works proceed by the Principal Contractor.  All portable fire extinguishing appliances shall be checked and serviced including recharging at regular intervals but at least once a month with a log kept of inspection time and action required.

No cylinders of liquid gas of any type are to be left within buildings (other than those designated safe storage areas) after normal working hours.

Flammable liquids within buildings must not exceed fifty litres and all must be removed to a safe place after normal working hours.

Fire breaks above false ceilings or service ducts are to be made good on completion of the immediate works, if disturbed.

The Principal Contractor will be required to work in accordance with HSG 168 and ‘Recommendations for Hot Work’ as issued by the Loss Prevention Council 1994
Hot work should not be carried out during one hour prior to normal shut down of the site at the finish of each working day.  Alternatively, careful inspection of all areas of the buildings to be undertaken one hour after hot work ceases and a log in a format agreed with the insurers shall be kept detailing these inspections.

The Principal Contractor should prepare his own fire and emergency plan which should be included with the Construction Phase Plan and displayed on site.
3.9
External works, phasing and site arrangements.
The external works will be the proposed pavement crossing, retaining walls patio area, landscaped areas and car park and entrance areas. There may be a requirement for working outside of the site boundaries for the making good of the public pavements

The phasing of the works will include the initial phase of general stripping out, asbestos removal and enabling works followed on by the fitout works.
3.10
‘No-go’ areas or other authorisation requirements for those involved in the project.


Not applicable
3.11
Confined spaces.

The Contractor shall clearly identify any areas that become apparent as a result of design development, in his Construction Phase Health & Safety Plan. The Contractor shall provide Method Statements and Risk Analysis to demonstrate that the stipulated methods of working have reduced the risks of illness, accident and or injury to minimum acceptable levels.

The Contractor shall also ensure that there is a safe means of access to and egress from a confined space to which a clearly identified method of ventilation must be identified.

The Contractor shall comply to the Guidance Note GS5 produced by the Health & Safety executive ‘Entry into Confined Spaces’ and the inspection procedures laid down in Part 4 of the CDM Regulations 2015.

3.12 Smoking.


No smoking will be allowed within the confines of the site.  Designated smoking areas may be provided within the Principal Contractor’s compound and must be carefully controlled, equipped with fire fighting equipment and receptacles for the safe disposal of smoker’s materials and inspected to guard against risk of fire. 

3.13 Parking restrictions.

There is parking available within the existing curtilidge of the site, however, parking should be restricted to the existing parking spaces and vehicles should not be parked in such a way so as to obstruct or cause a risk to vehicles and pedestrians using the shared access routes.    
Details of proposed areas for contractor’s parking should be indicated on the Site Layout Plan.
4.0       ENVIRONMENTAL RESTRICTIONS AND EXISTING ON-SITE RISKS

4.1
Boundaries and access 

The site boundaries are indicated on the Architects drawings including the site access position.
Access to the site will be via the existing vehicle & pedestrian access to the site. The Principal Contractor shall include detailed procedures within the Construction Phase Plan with respect to site access/egress & shall adopt all necessary practicable precautions to safeguard third parties & how delivery and pedestrian traffic will be integrated with site traffic. 
The boundaries of the site are to include the whole of the proposed building area and other external areas indicated on the site plan. 
There are no traffic or pedestrian routes across the site and the Principal Contractor is to give due consideration to the pedestrian areas to the perimeter of the site and entrances to the surrounding buildings. 
The Principal Contractor shall establish the nature of pedestrian routes and vehicular carriageways adjacent to the site and shall consider risks to third parties and include adequate protection as required to the Crimsworth Avenue elevations.
4.2
Restrictions on deliveries or waste collection or storage.

The Principal Contractor shall describe in a Method Statement his proposals for controlling waste on site and disposal of controlled waste. This should make reference to disposal to a registered tip and the documentation required to comply with local bylaws and statutory requirements
Waste storage on site outside any compound area should feature lockable covers outside of the working day.

4.3
Adjacent land uses.

The site lies on Crimsworth Avenue . The adjacent properties are other residential properties. The sites access lies on Crimsworth Avenue a residential road position and all will be in operation for the whole of the contract period. 
4.4
Existing storage of hazardous materials.


There will be no existing hazardous materials left on site.
4.5
Location of existing services particularly those that are concealed – water, electricity, 
gas etc.



There are services running alongside the site boundaries and within the car parking areas serving the existing buildings. Copies of the Authorities known services are held in later appendices of this plan.
4.5
Location of existing services particularly those that are concealed – water, electricity, 
gas etc.



The position & depth of the cables & pipes are indicative only & should be located using locating equipment prior to excavations commencing There may also be other un-marked services crossing the site. 

Therefore prior to excavation works, and drainage works commencing, a survey of the site will be carried out with a CAT and Genny to determine the presence and location of buried services local to the buildings and site. 
All live services found will be clearly marked by pins, signs, etc. Information on buried services will also be included in the site induction procedure. The known existing services relating to this site are indicated on a drawing referred to above.

During the works, continued use of electricity for power tools and lighting may require temporary wiring, which must comply with construction regulations.

4.6
Ground conditions, underground structures or water courses where this may affect 
the safe use of plant, e.g. cranes, or the safety of groundworkers.

A site investigation report has not been carried out for this stage of the works.
4.7
Information about existing structures.

There are no existing structures.
4.8
Previous structural modifications.
Not applicable
4.9
Fire damage, ground shrinkage, movement or poor maintenance which may have 
adversely affected the structure.

Not applicable.
4.10
Difficulties relating to plant and equipping the premises.


There are no known difficulties relating to plant or equipment, although the site is on a busy residential cul de sac opposite residential buildings.
4.11
Health and Safety information contained in earlier design, construction or ‘as-built’ 
documents.


An existing health & safety file or as built information was not available at the time of preparing this plan
4.12
Asbestos and Client surveys.

An asbestos survey has not been carried out
If during the course of the works any suspected asbestos or other toxic material is encountered the Principal Contractor is to take appropriate measures to prevent further hazard and should contact the Contract Administrator.

An existing services survey was not carried out 
4.13
Contaminated land, including results of surveys.

In view of the historical land use localised soil contaminants are not expected to be present on site. 
4.14
Existing structures containing hazardous materials.

No hazardous materials have been identified
4.15
Health risks arising from Client’s activities.


No activities will take place during the construction period.
5
SIGNIFICANT DESIGN AND CONSTRUCTION HAZARDS
5.1
Significant design assumptions and suggested work methods, sequences or other 
control measures.

It is a duty under the CDM Regulations 2015 and Health & Safety legislation that any contractor shall:

a. Identify and assess the risks in the proposed work.

b. Provide relevant Method Statements for approval.

c. Ensure proper induction in site rules for any person working on or visiting the 
site.

d. Undertake pro-active and re-active monitoring in order to maintain safety 
and health standards above statutory levels.

The Principal Contractor is reminded that close co-operation, liaison and pro-active planning of construction activities which impact on workers and other alike is essential, and in the event of a failure of risk control identified where injury or damage is considered imminent, the Principal Designer reserves the right to issue an instruction to immediately stop the activity until adequate measures and precautions are in place, at no cost to the Client.  
The design of the Contractor’s temporary structures such as scaffolding and any site modification to already erected structures will be undertaken by a competent specialist taking into account all circumstances of these particular works.

Scaffold, welfare and site office accommodation, site fencing and hoarding, signage, crane installation.
5.2
Arrangements for co-ordination of on-going design work and handling design 
changes.

If a design is prepared or developed on an ongoing basis, or if unforeseen circumstances require the Designer, Principal Contractor, or other contractors to make significant alterations to the design, the Principal Designer must be informed as soon as possible, ideally for consideration and acceptance before execution of the work.

Further design information will be generated in respect of 
Floors, 
Steelwork

Staircases 
Roof

Windows and external doors
Mechanical and Electrical Installations

Copies of drawings or information for Building Regulations approval or for the co-ordination of the work by the Architect will be required sufficiently in advance of the site construction.  These drawings and supporting information must relate to all connections to existing site services.  Full records of these altered or new services must be retained for the Health & Safety File.

5.3
Information on significant risks identified during design.

Successful risk management relies upon a systematic approach to the identification of hazards and risks and the pro-active allocation of resources to eliminate, reduce or control them.

The Principal Contractor will set out a system to successfully manage hazards and risks as set out in introduction clauses.  This will need to include CDM Regulations contained in Regulations 4, 9 and 39.  The principal of prevention in the Guidance on Regulations Appendix 1 should be embodied in the Principal Contractor’s management of the works.

Construction hazards of a routine and regular nature are not listed here as they should be known to a competent Principal Contractor.  However, some examples of potential hazards are given below:
Construction stage hazards & risks:
· Working at heights
· Traffic strategy and crossing footpaths
· Lifting operations
· Fire control
· Electrical installations including temporary installations
· Plant and work equipment

· Work beyond the site boundary

· Fire and hot works

· Noise, dust and vibration

· Generation of waste

· Health & Environment

· Manual handling

· Buried services

· Stability of unfinished structures

· Site vehicles

· Security and prevention of unauthorised entry
· Windows and glazing

· Means of escape

· Fragile materials 

· Scaffolding 
· Welfare facilities and temporary services provision
5.3
Information on significant risks identified during design.

Residual Risks: (to be outlined further in the Health and Safety File and Operation and Maintenance Manuals for the project)

· Working at heights
· Roof works and fragile materials
· Access for maintenance
· Window cleaning
· Maintaining emergency systems
· Equipment servicing
5.4
Materials requiring particular precautions.

Any operations involving chemical preparations, permitted by the specifications, shall be carried out by qualified persons.

The Principal Contractor shall be deemed to have carried out any assessment necessary of all materials specified to satisfy the Control of Substances Hazardous to Health Regulations.

The following materials and hazards have been identified as having particular health and safety implications:
Adhesives, sealant primers, cleaning solution and solvent, cartridge mastics containing silicone, polysulphides or acetic acid and specialist paint systems. 

 The risk from these products may include skin irritation, eye irritation, respiratory tract irritation, contact sensitisation.  The Principal Contractor shall obtain manufacturer’s Health and Safety Data Sheets and provide such ventilation measures, safe electrical equipment and other measures as required to carry out the above works in compliance with all health and safety legislation.



Substances hazardous in contact with the skin and mucous membranes typically include:

Brick, stone, plaster dust

Cement

Paints, varnishes, lacquers, stains

Acids

Alkalis

Acrylic and formaldehyde resins

Chromates (in primer paints, cement)

Petrol, white spirit, thinners

The importance of personal cleanliness should be emphasised together with the provision of appropriate gloves, barrier creams and skin conditioning creams.

Inhalation Hazards

Welding fumes

Man made mineral fibres

Silica and quartz dust arising from ground works, concrete scabbling etc.

Isocyanates (present in rigid insulation foams, paints, varnishes, adhesives)

Solvents (in paints, paint strippers, mastics, glues, surface coatings, etc).

Precautions may require forced ventilation, local extraction together with appropriate training and personal protective equipment.

5.4
Materials requiring particular precautions.

Contact Hazards

Cement

Treated timber

Treated metal work

Concrete

Highly Inflammable Materials
Great care needs to be taken in the use of highly inflammable materials during construction processes along fire escape routes (including corridors and staircases/staircase doors and final exits). 

Storage of hazardous materials
Where hazardous substances are to be stored, handled, used or produced as a result of the contractors activities, the contractor must take all necessary steps to ensure that exposure to these substances is kept to a minimum, and in any case below the exposure limits quoted in the Environmental Health Guidance Note 40. Activities must be conducted in such a way to ensure that the health & safety of operatives or any other person is not put at risk.
6

THE HEALTH AND SAFETY FILE


The project end files will consist of the following:

The Health and Safety File:
The Health and Safety File must be produced in accordance with CDM 2015, regulation 12.  The Client has confirmed that 1 no. hard copy and 1 no. electronic copy of the file are required. 

The Health and Safety File is a record of information for the end user that focuses on health and safety.  The information it contains will alert those who are responsible for the structure and plant of the significant health and safety risks that will need to be dealt with during subsequent use, modifications to construction, maintenance and in some cases eventual demolition of the building.

From the handing over of the file, the client must take steps to keep it up to date (regulation 17, clause 3 (a) and (b)).  The Health & Safety File must be handed over to the new owner, should the freehold interest be transferred.  The Designers must supply a list of key drawings and other information such as structural calculations or details where this could have a bearing on future modifications for inclusion in the file. 

The Principal Contractor is required to obtain/retain adequate and sufficient health and safety information throughout the construction phase, including information from subcontractors relating to the Health and Safety File.  


This specific information, as noted above, shall be passed to the Principal Designer in a timely manner (see 1.12) with all information being received 2 weeks before completion.  The Principal Designer will then assemble the File and hand to the Client.
The H&S File contents/requirements are also prescribed in an extract from the Guidance on the Regulation which will be sent to the entire project team,


Schedule of Project Information (this list is not exhaustive):
(a)
a brief description of the work carried out and project start and end dates;

(b)
any residual hazards which remain and how they have been dealt with (for 
example surveys information concerning asbestos; contaminated land; 
water bearing strata; buried 
services etc);

(c)
key structural principles (for example, bracing, sources of substantial stored 
energy – including pre- or post-tensioned members) and safe working 
loads for floors and roofs, particularly where these may preclude placing 
scaffolding or heavy machinery there;

(d)
hazardous materials used (for example lead paint; pesticides; special 
coatings which should not be burnt off etc);

(e)
information regarding the removal or dismantling installed plant and 
equipment (for example any special arrangements for lifting, order or other 
special instructions for dismantling etc);

(f)
health and safety information about equipment provided for cleaning or 
maintaining the structure;

(g)
the nature, location and markings of significant services, including 
underground cables; gas supply equipment; fire-fighting services etc;

(h)
information and as-built drawings of the structure, its plant and equipment 
(for example, the means of safe access to and from service voids, fire 
doors and compartmentalisation etc).

Building  Manual and Services Operation and Maintenance Manuals:
As set out in the Contract Prelims.  The Principal Contractor is to liaise with all relevant sub-contractors and suppliers to compile sufficient information to the client upon handover.  Designers will be required to include As Built / As Installed drawings and Specifications, as required.  

Please note:  The Principal Designer deals only with the statutory Health & Safety File information.  Any related Building and Services O&M Manuals are a contractual requirement and should be checked by the relevant consultants.
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