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SITE-SPECIFIC 
 RISK ASSESSMENT

	SITE ADDRESS (inc. postcode):
	Risk Assessor:
	

	
	Date:
	

	Job Description

	

	WAH ASSESSMENT
	         WAH
JUSTIFICATION:
	

	

	All work from Ground Level
	



	

	Temporary Access Platform
	

	

	Climbing/Personal fall protection
	

	BIOSECURITY RISK ASSESSMENT – 
Is a concerning Pest & Disease (P&D) present or suspected on or adjacent to site?  See 3.4
	


	

	DISPOSAL OF ARISINGS / SPECIFIC REQUIREMENTS:
	

	

	OPERATIVES COMPETENT TO USE EQUIPMENT ISSUED/CARRY OUT OPERATION SPECIFIED?
	Yes
	No


Risk Assessment continued overleaf/........


EMERGENCY CONTINGENCIES office number 01257 231 590

	Nearest A&E (inc. postcode)
	Site postcode / Grid Reference

	
	

	Designated Climber and Rescuer
	Names: 

	Havs Monitoring
	Are all staff using Vibrating tools wearing havs watch   
                       Yes:              No:

If No please State why:








SITE-SPECIFIC RISK ASSESSMENT – Cont
	
Generic Assessment, and Assessment Number
	Relevant? (tick)
	Generic Assessment, and Assessment Number
	Relevant? (tick)

	WEATHER
	
SITE CONSIDERATIONS

	Record any adverse change to the weather during the task.
	

	
	

	ENVIRONMENTAL CONSIDERATIONS
	
	
	Work site – Common factors
	10.2.1
	

	Proposed work adjacent to watercourse
	10.3.1
	
	Disease and infection
	10.2.2
	

	Proposed work adj. to protected spp. or habitat
	10.3.2
	
	Power lines
	10.2.3
	

	Excessive noise or dust
	10.3.3
	
	Other way leaves
	10.2.4
	

	Bio-Security
	10.3.4
	
	Buildings/obstructions
	10.2.5
	

	OPERATIONS
	Roads/footpaths/public areas
	10.2.6
	

	Chainsaws – common factors
	10.4.1
	
	Sensitive/emotionally charged locality
	10.2.7
	

	Tree climbing/rope access - common factors
	10.4.2
	
	Site Security
	10.2.8
	

	Chainsaw in tree - common factors
	10.4.3
	
	Other (e.g. over water, hospital or school grounds etc.)
	

	Branch removal
	10.4.4
	
	MACHINERY

	Lowering equipment
	10.4.5
	
	Brushwood chipper
	10.5.1
	

	Tree felling
	10.4.6
	
	Stump grinder
	10.5.2
	

	Delimbing and cross cutting
	10.4.7
	
	Winch
	10.5.3
	

	Storm damage
	10.4.8
	
	Mobile Elevated Work Platform
	10.5.4
	

	Pesticide application
	10.4.9
	
	Crane
	10.5.5
	

	TRANSPORT
	
	
	Hydraulic loading
	10.5.6
	

	Vehicles
	10.6.1
	
	Bandit Wood Chipper
	10.5.7
	

	Moving Vehicles Coupling trailers
	10.6.2
	
	Plant Movements
	10.5.8
	

	Transportation on Clients site
	10.6.3
	
	Excavation work 
	10.5.9
	

	Reversing
	10.6.4
	
	Fuel storage
	10.5.10
	

	Traveling to site
	10.6.5
	
	Fuel storage
	10.5.11
	

	Loading/Offloading trailers &Hook skip
	10.6.6
	
	Fuelling of plant
	10.5.12
	

	Work at Height
	10.6.7
	
	Loading fuel into fuel stores
	10.5.13
	

	Unsecure Loads
	10.6.8
	
	
	
	

	Use of winch/tow vehicle to load
	10.6.9
	
	
	
	

	Loading unpowered Equipment
	10.6.10
	
	
	
	

	Chains Straps & load tensioners
	10.6.11
	
	
	
	

	CIVILS RAMS

	Tarmac repairs/replace
	MMS001
	
	Door hardware repair/replace
	MMS016
	

	Fencing
	MMS002
	
	White lining (Platforms)
	MMS017
	

	Flagging, block paving, concreting
	MMS003
	
	White lining (carparks)
	MMS018
	

	Soakaway clearance
	MMS004
	
	Graffiti removal (water Jet)
	MMS019
	

	Anti-Slip repairs
	MMS005
	
	Graffiti removal (painting)
	MMS020
	

	Drainage Clearance
	MMS006
	
	Vegetation control
	MMS021
	

	Manhole repairs
	MMS007
	
	Brick and block work
	MMS022
	

	Water leak investigations
	MMS008
	
	Excavations
	MMS023
	

	Pitch roof and gutter works
	MMS009
	
	Internal plastering
	MMS024
	

	Flooring
	MMS010
	
	Copes and tactile works
	MMS025
	

	Shutter door repairs
	MMS011
	
	Tiling
	MMS026
	

	Lightbulb replacing
	MMS012
	
	Electrical works
	MMS027
	

	Abacus Lighting column repairs
	MMS013
	
	Glazing works
	MMS028
	

	Plumbing and gas fitting
	MMS014
	
	Painting works
	MMS029
	

	Joinery works
	MMS015
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	




Arb Methods

	Use of chainsaw
	ArbMS 00
	
	Annual tree inspection
	ArbMS 01
	

	Chippings arising
	ArbMS 02
	
	Climbing inspection
	ArbMS 03
	

	Climbing
	ArbMS 04
	
	Crown lifting
	ArbMS 05
	

	Crown reduction
	ArbMS 06
	
	Crown thinning
	ArbMS 07
	

	Dead wooding
	ArbMS 08
	
	Dismantling
	ArbMS 09
	

	Felling
	ArbMS 10
	
	Pollarding
	ArbMS 11
	

	Removal and replanting of trees
	ArbMS 12
	
	Stump grinding
	ArbMS 13
	

	Stump removal
	ArbMS 14
	
	Suckers, basal and epicormic growth
	ArbMS 15
	

	Veteran tree management
	ArbMS 16
	
	Barge works
	ArbMS 17
	

	Excavator with attachments 
	ArbMS 18a
	
	Lifting equipment 
	ArbMS 19
	

	Mewp
	ArbMS 20
	
	Trees>150mm dbh: overhanging
	ArbMS 21
	

	Trees>150mm dbh: in falling distance no overhang 
	ArbMS 22
	
	Dead trees>150mm dbh overhang
	ArbMS 23
	

	Dead trees>150mm no overhang or in fall distance
	ArbMS 24
	
	Scrub/trees<150mm within fall distance of line
	ArbMS 25
	

	Scrub/trees<150mm overhanging line
	ArbMS 26
	
	Saplings/shrubs/understorey vegetation
	ArbMS 27
	

	Conductor rail
	ArbMS 28
	
	Overhead line equipment
	ArbMS 29
	





Continue site specific details on the sheet that follows 

SITE-SPECIFIC RISK ASSESSMENT – Cont

List here the specific hazards/considerations of the site that pose a risk which needs to be controlled/ managed and then say how this will be achieved? (Example below)

	HAZARDS
	Risk
Level
	CONTROLS
	Residual risk

	Tree has pathogens or known defects that have not been notified prior to commencement of works.
To be completed on site prior to starting works
	
	Stop works and notify Client and Manager about change of work method required. 
	

	

















	
	
	


Cont. on separate sheet if needed or develop further ‘generics’ for regular hazards/issues & add to list below

	
Site Specific Risk Assessment Completed by
	

	Site Safety Coordinator – name
	

	Date
	Name / Sign:
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