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Cornthwaite Tree Care, Unit 10 Crosse Hall Works, Crosse Hall Street, Chorley PR6 0QQ

___________________________________________________________________________________________________________________________________________

10.6
USE of Transport Vehicles 
	Ref
	Hazard
	Risks
	Persons & item’s involved
	Initial Risk
	Industry best practice/guidance
	Date issued

(to those at risk)
	Control measures
	Residual risk

	10.6.1
	Vehicles


	Yard access/egress and manoeuvring  
	Staff and others may suffer serious, possibly fatal, injury if struck by a vehicle

Vehicle, equipment and property damage.
	Remote Unlikely But Conceivable -3

	Machines parked in machine store with designated 
Safe, well-marked pedestrian routes

All areas well lit

Carryout all pre-start checks paying attention to cleanliness of windows and mirrors. 
	Workplace Transport Safety
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	Management system where practicable and staff to be aware of vehicle movements at all times. The busy times were most movements happen are between

(07:00-08:00 & 15:00-16:00)

Warning Signs
High-visibility worn by all entering the yard and store area.

	Acceptable Risk
2- Minor

	10.6.2
	Moving Tractor or Vehicles & trailer 

Combination 


	Coupling and uncoupling of tractor or vehicles  with trailers


	Drivers/others may suffer serious crush injuries if trapped 
	Remote Unlikely But Conceivable -3

	Drivers follow safe systems of work for coupling/uncoupling


	Workplace Transport Safety
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	Spot checks to ensure drivers following safe system of work
Ensure  workers 
are trained in safe 
system of work 


	Acceptable Risk
2- Minor

	10.6.3
	Transportation to or through client’s site
	Collision
	Injury to persons

Damage vehicles
	Remote Unlikely But Conceivable -3


	Trained certified operatives Flashing Beacons

Observing site  speed limit
	Workplace Transport Safety
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	Use designated maintained haul routes

Inspect Condition of site haul routes
	Tolerable

   1-Low

	10.6.4
	Transportation
	Reversing of Trailers 
	Injury to persons
Damage vehicles
	Remote Unlikely But Conceivable -3


	Use of Reversing siren & Flashing Beacons reversing to be carried out under instruction of vehicle movement supervisor
	
	Staff to assist with keeping unauthorized personnel out of area while vehicles are movement into or out of site area
	Tolerable

   1-Low

	10.6.5
	Traveling to and from site
	Collision with vehicles pedestrians and infrastructure
	General public, Vehicles , Buildings & Infrastructures
	Remote Unlikely  But Conceivable -3


	Vehicles maintained and comply with road traffic act 
Operator trained and holds the relevant licence 
Use the principals of the Highway Code.
	
	Vehicle checked for faults daily with daily check sheet completed and archived
	Tolerable

   1-Low

	10.6. 6
	Uncontrolled Movement of items while loading
	Loading or Off Loading or items  from low loader/trailers/hook trailer
	Injury to operators

Damage vehicles
	Remote Unlikely But Conceivable -3


	Driver to engage dead man brake and stop engine when leaving the machine 

Vehicle driver to be trained & competent in all methods of loading / unloading of plant and equipment using all ramps

Vehicle driver to be trained & competent in all methods of loading / unloading various items using Manual handling & Mechanical methods
Driver to be trained and competent in loading and unloading HOOK SKIPS
	
	Trained operatives to follow direction issued by delivery vehicle driver if assisting during loading / off loading operations over the rear of the trailer using the ramps.

All supplied ramps must be used during loading / off loading if ramps are missing do not attempt to load using other methods
	Acceptable Risk
2- Minor

	10.6.7
	Falls  from height
	Loading or Off Loading plant and Items 
	Injury to operators


	Remote Unlikely But Conceivable -3


	Trained operatives to follow correct 3 points of contact method when entering and exiting equipment 


	Fall from vehicles.
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	Ensure low-loader/trailer bed is as clean as practicable and free of trip hazards

PPE (suitable footwear with adequate tread
	Tolerable

Low-1

	10.6.8
	unsecure Load
	Loss  of Load


	General public, site staff, Vehicles , Buildings & Infrastructures  Contamination of site area and highway
	Remote Unlikely But Conceivable -3


	All loads must be secured by the driver using the appropriate restraints, straps or Chains. 

Driver to check load and vehicle before moving off


	
	Driver to monitor, load’s during  transit and check restreints periodically 
	Tolerable

Low-1

	10.6.9
	Use of winch or towing vehicle
	Mechanical failure to winch, tow vehicle, winch rope or tow rope due to snagging of load during movement
	Collision or whip Injury/fatality to persons or damage vehicles
	Remote Unlikely But Conceivable -3


	Operator to visually Inspect winch, tow rope and load prior to operation start 

Operator to monitor progress of load during operation 

If close inspection is required 

operation must cease and stored energy released from towing/winching accessories 
	
	Area to be cleared of personnel during winching or towing operation.

Operation to stop if there is any unaurthorizerd access to loading area. 
Area to be cleared of personnel before operation can resume. 
	Acceptable Risk
2- Minor


	10.6.10
	Loading

 unpowered equipment
	Use of winch or towing/Pushing  to load  

 unpowered vehicle
	Collision or whip Injury/fatality to persons or damage vehicles
	Remote Unlikley But Conceivable -3


	Trained operatives to follow direction issued by delivery/collection vehicle driver during off loading/loading operations over the rear of the trailer using the ramps.

 Area to be cleared of personnel during winching or towing operation

 If close inspection is required 

operation must cease and stored energy released from towing/winching accessories
	
	Area to be cleared of personnel during winching or towing operation.

Operation to stop if there is any unaurthorizerd access to loading area. Area to be cleared before operation can resume.
	Acceptable Risk
2- Minor

	10.6.11
	Chains/straps and Load  Tensioners 
	Securing loads
	Trap/Crush injury to hands and fingers of operator or staff
	Remote Unlikley But Conceivable -3


	Trained operatives to follow direction issued by delivery/collection vehicle driver during securing of loads. 
	
	Agree and Use good communication methods while securing loads
	Tolerable

Low-1
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