
	RISK ASSESSMENT

Dry Lining and Plastering
	Ref: D004

	
	Page 1 of 2

	EMPLOYER:     Harry Brook & Son Limited

	LOCATION NBS 74 king street Manchester M2 4NJ

	ASSESSED BY:   Carl Hudson
	DESIGNATION:    H & S Director

	LEGEND:   Likelihood and Severity:- 1 = Low  2 = Medium  3 = High

   Risk Rating (L x S):-  1-4 = Low (Acceptable)  6 = Medium (Consider further controls)  9 = Unacceptable (Do not proceed)

	SIGNIFICANT HAZARDS IDENTIFIED:Give a brief description of what could be reasonably expected to cause significant harm and how that harm may arise.
	RISK ASSESSMENT

	
	UNCONTROLLED
	CONTROLLED

	
	L
	S
	RR
	L
	S
	RR

	Inhalation of plaster dust – causing acute or chronic harm
	2
	3
	6
	1
	3
	3

	Use of electric mixing tool – electric shock and entanglement or contact with mixing blade
	2
	3
	6
	1
	3
	3

	Falls from height – when plastering ceilings, high walls, etc.
	2
	3
	6
	1
	3
	3

	Mechanical movement of plasterboard packs (72 boards of 2440 x 1220 weight 1750kg). Use of mobile plant in restrictive area – persons and structures being struck
	2
	3
	6
	1
	3
	3

	Manual handling of individual boards – each board weights 24.3kg and is unwieldy
	2
	2
	4
	1
	2
	2

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	PERSONS AT RISK
	Y/N
	DETAIL

	EMPLOYEES
	Y
	Those involved in the activities 

	CONTRACTORS
	Y/N
	

	MEMBERS OF PUBLIC
	Y/N
	

	OTHERS
	Y/N
	

	CONTROL MEASURES:

	1.
	Before commencing plastering operations, the COSHH assessment and safety data sheet for plaster must be checked.

	2.
	Plaster must be mixed in well ventilated areas. Use PP3 dust mask where necessary,

	3.
	Operatives must practice good hygiene – wash regularly and thoroughly.

	4.
	See separate assessment for use of electric tools.

	5.
	See separate assessment for use of ladders.

	5.
	See separate assessment for use of Mobile Scaffold Towers.

	6.
	Packs must be set down in convenient locations near to the work area. The set down location must be level and easily accessible by persons on foot (no slips and trips hazards).

	7.
	Routes between the work area and the packs of boards must be clean, level and free of obstruction.

	8.
	Only one plasterboard sheet at a time must be manually lifted.

	9.
	Plasterboards should preferably be handled using two-person lifting. Single person lifts are acceptable only if specific manual handling instruction/training is given and the size of the board can be easily managed by the operative.

	10.
	Repetitive lifting of boards must be avoided. Plan work to mix work activities by carrying minimum numbers of boards and then changing to lining or plastering activities.

	
	

	
	

	
	

	
	

	Remember:

Always check in your safety manual for Company safety procedures and systems of work.

Refer to other assessments for activities connected with this assessment.


	RISK ASSESSMENT

Dry Lining and Plastering
	Ref: D004

	
	Page 2 of 2

	ADDITIONAL CONTROL MEASURES: (Review at workplace and add any additional specific controls required)


	PERSONAL PROTECTIVE EQUIPMENT:

The following PPE will be required for the work activities stated. Ensure the correct TYPE of PPE is selected.

	Head Protection
	(
	Eye/Face Protection
	(
	Hearing Protection
	
	Hi-visibility Clothing
	
	Gloves
	

	Foot Protection
	(
	Safety Clothing
	(
	R.P.E.
	
	Fall Arrest 
	
	
	

	REVIEW AND MONITORING:

Review in light of further information becoming available or a change in conditions/circumstances.



	INFORMATION TO BE PROVIDED TO EMPLOYEES:

Information contained in this and other related assessments.

Operator training.

Manual handling instruction.



	The following persons have received the information contained in this assessment:

	Name
	Date
	Initial
	Name
	Date
	Initial

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	SIGNED BY ASSESSOR:
Iain Brook
	Date:
June 2020

	


	RISK ASSESSMENT

Use of Hand Tools
	Ref: H001

	
	Page 1 of 2

	EMPLOYER:     Harry Brook & Son Limited

	LOCATION      NBS 74 king street Manchester M2 4NJ

	ASSESSED BY:   Carl Hudson
	DESIGNATION:    H & S Director

	LEGEND:   Likelihood and Severity:- 1 = Low  2 = Medium  3 = High

   Risk Rating (L x S):-  1-4 = Low (Acceptable)  6 = Medium (Consider further controls)  9 = Unacceptable (Do not proceed)

	SIGNIFICANT HAZARDS IDENTIFIED:

Give a brief description of what could be reasonably expected to cause significant harm and how that harm may arise.
	RISK ASSESSMENT

	
	UNCONTROLLED
	CONTROLLED

	
	L
	S
	RR
	L
	S
	RR

	Injuries to eyes caused by flying particles.
	2
	3
	6
	1
	3
	3

	Injury to hands, feet and body from contact with tool or work piece.
	2
	2
	4
	1
	2
	2

	Sprains and strains caused by using hand tools incorrectly.
	2
	2
	4
	1
	2
	2

	Injury causes by tripping over tools (due to poor housekeeping).
	2
	2
	4
	1
	2
	2

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	PERSONS AT RISK
	Y/N
	DETAIL

	EMPLOYEES
	Y
	Employees undertaking activity

	CONTRACTORS
	Y/N
	

	MEMBERS OF PUBLIC
	Y/N
	

	OTHERS
	Y/N
	

	CONTROL MEASURES:

	1.
	Ensure that hand tools are not used for any other than their intended purpose (e.g. do not use a screwdriver as a chisel).

	2.
	Operatives must carry out visual checks of hand tools before their first use each day. Damaged or dangerous tools must not be used.

	3.
	Eye protection MUST be used whenever work is carried out using cold chisels, drills, sanders or any other tools where there is a risk of flying particles.

	4.
	Open-bladed knives, screwdrivers and other sharp tools must not be carried in pockets or in any manner which could cause injury to the user or others.

	5.
	In flammable atmospheres or where highly flammable substances may be present, only non-ferrous (spark free) tools must be used.

	6.
	Sharpening is a skilled task and must only be carried out by trained and authorised persons.

	7.
	Tools must not be left lying about but returned to storage after use.

	8.
	Common faults which must be checked for include:

· mushroomed heads on chisels

· loose and damaged hammer and file handles

· splayed jaws on open-ended spanners

· damaged pick and shovel handles

· damaged screwdriver blades.

	9.
	Periodic thorough examinations are recommended, with records kept.

	10.
	Certain tasks using hand tools can result in high sound pressures – hearing protection must be worn if carrying out sustained hammering or other noisy tasks.

	Remember:

Always check in your safety manual for Company safety procedures and systems of work.

Refer to other assessments for activities connected with this assessment.


	RISK ASSESSMENT

Use of Hand Tools
	Ref: H001

	
	Page 2 of 2

	ADDITIONAL CONTROL MEASURES: (Review at workplace and add any additional specific controls required)




	PERSONAL PROTECTIVE EQUIPMENT:

The following PPE will be required for the work activities stated. Ensure the correct TYPE of PPE is selected.

	Head Protection
	
	Eye/Face Protection
	(
	Hearing Protection
	(
	Hi-visibility Clothing
	(
	Gloves
	(

	Foot Protection
	(
	Safety Clothing
	
	R.P.E.
	
	
	
	
	

	REVIEW AND MONITORING:

Review in light of further information becoming available or a change in conditions/circumstances.



	INFORMATION TO BE PROVIDED TO EMPLOYEES:

Information contained in this assessment.

Operator training.



	The following persons have received the information contained in this assessment:

	Name
	Date
	Initial
	Name
	Date
	Initial

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	SIGNED BY ASSESSOR:
Iain Brook
	DATE
June 2020


	


	RISK ASSESSMENT

Manual Handling and Lifting
	Ref: M002

	
	Page 1 of 2

	EMPLOYER:     Harry Brook & Son Limited

	LOCATION      NBS 74 king street Manchester M2 4NJ

	ASSESSED BY:   Carl Hudson
	DESIGNATION:    H & S Director

	LEGEND:   Likelihood and Severity:- 1 = Low  2 = Medium  3 = High

   Risk Rating (L x S):-  1-4 = Low (Acceptable)  6 = Medium (Consider further controls)  9 = Unacceptable (Do not proceed)

	SIGNIFICANT HAZARDS IDENTIFIED:

Give a brief description of what could be reasonably expected to cause significant harm and how that harm may arise.
	RISK ASSESSMENT

	
	UNCONTROLLED
	CONTROLLED

	
	L
	S
	RR
	L
	S
	RR

	Back strain, slipped disc, hernias due to incorrect handling or lifting
	2
	3
	6
	1
	3
	3

	Lacerations, crushing of hands or fingers
	2
	3
	6
	1
	3
	3

	Bruised or broken toes or feet 
	2
	3
	6
	1
	3
	3

	Tenosynovitis, various sprains and strains
	2
	3
	6
	1
	3
	3

	PERSONS AT RISK
	Y/N
	DETAIL

	EMPLOYEES
	Y
	Operative involved in activity

	CONTRACTORS
	Y/N
	

	MEMBERS OF PUBLIC
	Y/N
	

	OTHERS
	Y/N
	

	CONTROL MEASURES:

	1.
	Ensure all operatives involved in manual handling operations are trained in the relevant procedures. Training will be based on the physical structure of the body and the effect of attempt to handle loads in various positions.

	2.
	Wherever possible use mechanical means to lift and transport items.

	3.
	Where use of mechanical means is impracticable, then sufficient persons must be available to lift the load and take into account the size, shape and weight of that load. Consideration will also be given to the path of the load and the immediate environment, e.g. floor conditions, lighting, access etc.

	4.
	Ensure items are correctly lifted with back straight and using the legs to raise yourself if the load is low. Use a good grip with the feet apart to hip width and one foot slightly in front of the other.

	5.
	Avoid twisting, stooping or reaching to left or deposit the load.

	6.
	Ensure that access areas are clean, clear and that the lighting is adequate.

	7.
	Wear suitable personal protective equipment, i.e. gloves, safety footwear equipment relevant to the working environment.

	8.
	Protect sharp edges.

	9.
	Avoid long lifts and if necessary change grip when the load is at waist height.

	10.
	Keep the load close to the body.

	11.
	Arrange storage so that the heaviest loads are in the most convenient position, i.e. from knee to shoulder range.

	12.
	For long distances arrange supports to allow the load to be placed for brief breaks. If possible, break the load down into smaller items. If possible, provide proper handles, handholds or use carrying devices to avoid the possibility of trapped fingers etc.

	13.
	Secure items which are loose to prevent the load shifting when being carried. Avoid carrying up and down steps.

	Remember:

Always check in your safety manual for Company safety procedures and systems of work.

Refer to other assessments for activities connected with this assessment.


	RISK ASSESSMENT

Manual Handling and Lifting
	Ref: M002

	
	Page 2 of 2

	ADDITIONAL CONTROL MEASURES: (Review at workplace and add any additional specific controls required)




	PERSONAL PROTECTIVE EQUIPMENT:

The following PPE will be required for the work activities stated. Ensure the correct TYPE of PPE is selected.

	Head Protection
	(
	Eye/Face Protection
	
	Hearing Protection
	
	Hi-visibility Clothing
	(
	Gloves
	

	Foot Protection
	(
	Safety Clothing
	
	R.P.E.
	
	Fall Arrest (in MEWP)
	
	
	

	REVIEW AND MONITORING:

Review in light of further information becoming available or a change in conditions/circumstances.



	INFORMATION TO BE PROVIDED TO EMPLOYEES:

Information contained in this assessment.

Site safety induction.

Manual Handling instruction (if applicable).


	The following persons have received the information contained in this assessment:

	Name
	Date
	Initial
	Name
	Date
	Initial

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	SIGNED BY ASSESSOR:
Iain Brook
	DATE:

June 2020

	


	RISK ASSESSMENT

Percussive Tools
	Ref: P003

	
	Page 1 of 2

	EMPLOYER:     Harry Brook & Son Limited

	LOCATION:     NBS 74 king street Manchester M2 4NJ

	ASSESSED BY:   carl Hudson
	DESIGNATION:    H & S Director

	LEGEND:   Likelihood and Severity:- 1 = Low  2 = Medium  3 = High

   Risk Rating (L x S):-  1-4 = Low (Acceptable)  6 = Medium (Consider further controls)  9 = Unacceptable (Do not proceed)

	SIGNIFICANT HAZARDS IDENTIFIED:

Give a brief description of what could be reasonably expected to cause significant harm and how that harm may arise.
	RISK ASSESSMENT

	
	UNCONTROLLED
	CONTROLLED

	
	L
	S
	RR
	L
	S
	RR

	Vibration white finger due to prolonged exposure
	3
	3
	9
	1
	3
	3

	Hearing impairment due to excessive noise levels
	3
	3
	9
	1
	3
	3

	Muscular skeletal disorders
	2
	3
	6
	1
	2
	3

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	PERSONS AT RISK
	Y/N
	DETAIL

	EMPLOYEES
	Y
	Operators

	CONTRACTORS
	Y
	Others in the vicinity

	MEMBERS OF PUBLIC
	Y/N
	

	OTHERS
	Y/N
	

	CONTROL MEASURES:

	1.
	Vibration dampening devices on tools are employed whenever possible.

	2.
	Anti-vibration and hand grips are used on tools.

	3.
	Vibration absorbent gloves are used as appropriate.

	4.
	Only trained and competent persons use tools.

	5.
	Task rotation or work share is adopted to reduce exposure to vibration. Check vibration assessment for maximum operating time for appropriate piece of equipment to be used.

	6.
	Tools are maintained in good working and according to manufacturers’ instructions.

	7.
	Records of inspection are kept.

	8.
	Regular flexing of fingers and hands is strongly recommended.

	9.
	Tool box talks are given on the subject of percussive tools.

	10.
	Noise assessment to be carried out as necessary. Suitable and sufficient ear defenders are used for the relevant action level.

	11.
	Persons using percussive tools during cold weather should keep warm when working.

	12.
	Records are kept for the monitoring or certifications, maintenance, training and inspections by competent persons.

	
	

	
	

	
	

	
	

	
	

	Remember:

Always check in your safety manual for Company safety procedures and systems of work.

Refer to other assessments for activities connected with this assessment.


	RISK ASSESSMENT

Percussive Tools
	Ref: P003

	
	Page 2 of 2

	ADDITIONAL CONTROL MEASURES: (Review at workplace and add any additional specific controls required)




	PERSONAL PROTECTIVE EQUIPMENT:

The following PPE will be required for the work activities stated. Ensure the correct TYPE of PPE is selected.

	Head Protection
	(
	Eye/Face Protection
	(
	Hearing Protection
	(
	Hi-visibility Clothing
	(
	Gloves
	(

	Foot Protection
	(
	Safety Clothing
	
	R.P.E.
	
	
	
	
	

	REVIEW AND MONITORING:

Review in light of further information becoming available or a change in conditions/circumstances.



	INFORMATION TO BE PROVIDED TO EMPLOYEES:

Information contained in this assessment.

Site safety induction



	The following persons have received the information contained in this assessment:

	Name
	Date
	Initial
	Name
	Date
	Initial

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	SIGNED BY ASSESSOR:
Iain Brook
	DATE:

May 2020 

	


	RISK ASSESSMENT

Portable Electrical Appliances
	Ref: P006

	
	Page 1 of 2

	EMPLOYER:     Harry Brook & Son Limited

	LOCATION NBS 74 king street Manchester M2 4NJ

	ASSESSED BY:   carl Hudson
	DESIGNATION:    H & S Director

	LEGEND:   Likelihood and Severity:- 1 = Low  2 = Medium  3 = High

   Risk Rating (L x S):-  1-4 = Low (Acceptable)  6 = Medium (Consider further controls)  9 = Unacceptable (Do not proceed)

	SIGNIFICANT HAZARDS IDENTIFIED:

Give a brief description of what could be reasonably expected to cause significant harm and how that harm may arise.
	RISK ASSESSMENT

	
	UNCONTROLLED
	CONTROLLED

	
	L
	S
	RR
	L
	S
	RR

	Damaged or poorly maintained electrical equipment resulting in electric shock, burns and possible death.
	2
	3
	6
	1
	3
	3

	Leads and fittings that are not maintained resulting in burns, electric shock and possible death.
	2
	3
	6
	1
	3
	3

	Trailing cables causing trip hazards resulting in moderate to severe injuries.
	2
	3
	6
	1
	3
	3

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	PERSONS AT RISK
	Y/N
	DETAIL

	EMPLOYEES
	Y
	Operatives engaged in activity

	CONTRACTORS
	Y/N
	

	MEMBERS OF PUBLIC
	Y/N
	

	OTHERS
	Y/N
	

	CONTROL MEASURES:

	1.
	All equipment is tested, inspected at regular intervals and a register kept of all appliances and test dates.

	2.
	Prior to use, electrical equipment including leads is checked for visible damage and removed if found to be defective.

	3.
	Only 110v power tools are used on site.

	4.
	Cables are suspended where possible and protected from trapping.

	5.
	Electrical equipment complies to relevant CENELEC standards.

	6.
	Equipment that is damaged is repaired before use and tested.

	7.
	Electrical equipment is not lifted by its cable and operatives are instructed not to do so.

	8.
	Only trained and competent persons may use electrical appliances.

	9.
	Supplies to electrical appliances are checked and RCD protection is used.

	
	

	
	

	
	

	
	

	
	

	Remember:

Always check in your safety manual for Company safety procedures and systems of work.

Refer to other assessments for activities connected with this assessment.


	RISK ASSESSMENT

Portable Electrical Appliances
	Ref: P006

	
	Page 2 of 2

	ADDITIONAL CONTROL MEASURES: (Review at workplace and add any additional specific controls required)




	PERSONAL PROTECTIVE EQUIPMENT:

The following PPE will be required for the work activities stated. Ensure the correct TYPE of PPE is selected.

	Head Protection
	(
	Eye/Face Protection
	(
	Hearing Protection
	(
	Hi-visibility Clothing
	(
	Gloves
	(

	Foot Protection
	(
	Safety Clothing
	
	R.P.E.
	
	
	
	
	

	REVIEW AND MONITORING:

Review in light of further information becoming available or a change in conditions/circumstances.



	INFORMATION TO BE PROVIDED TO EMPLOYEES:

Information contained in this assessment.



	The following persons have received the information contained in this assessment:

	Name
	Date
	Initial
	Name
	Date
	Initial

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	SIGNED BY ASSESSOR:
Iain Brook
	DATE:

June 2020

	


	RISK ASSESSMENT

Mobile Scaffold Tower (MST).
	Ref: S003

	
	Page 1 of 2

	EMPLOYER:     Harry Brook & Son Limited

	LOCATION NBS 74 king street Manchester M2 4NJ

	ASSESSED BY:   Carl Hudson
	DESIGNATION:    H & S Director

	LEGEND:   Likelihood and Severity:- 1 = Low  2 = Medium  3 = High

   Risk Rating (L x S):-  1-4 = Low (Acceptable)  6 = Medium (Consider further controls)  9 = Unacceptable (Do not proceed)

	SIGNIFICANT HAZARDS IDENTIFIED:

Give a brief description of what could be reasonably expected to cause significant harm and how that harm may arise.
	RISK ASSESSMENT

	
	UNCONTROLLED
	CONTROLLED

	
	L
	S
	RR
	L
	S
	RR

	Falls of persons from MST causing fractures, bruising and/or internal injuries
	3
	3
	9
	1
	3
	3

	Falls of materials from MST striking persons below
	2
	2
	4
	1
	2
	2

	Striking overhead cables with MST – electric shock
	2
	3
	6
	1
	3
	3

	Overloading or incorrect erection or poor ground conditions
	3
	3
	9
	1
	3
	3

	PERSONS AT RISK
	Y/N
	DETAIL

	EMPLOYEES
	Y
	Operatives engaged in activity

	CONTRACTORS
	Y
	Operatives within the vicinity

	MEMBERS OF PUBLIC
	Y
	Persons within the vicinity of works

	OTHERS
	Y/N
	

	
	
	

	CONTROL MEASURES:

	1.
	All scaffold towers to be constructed by competent persons, with guardrails and toeboards provided.

	2.
	Inspect MSTs daily and make a written record at least every 7 days.

	3.
	Consider MST specification with regard to ground conditions, height restrictions and overhead obstructions (if present).

	4.
	Ground conditions are level and firm and when necessary metal base plates and timber sole boards are used and outriggers deployed.

	5.
	Ladder access should be internal and fixed to the narrowest side.

	vv6.
	Tower scaffolds are loaded in accordance with the manufacturers’ instructions.

	7.
	Edge protection is used – guard rails and toe boards at platforms from which a person could fall 2m or more and below 2m where injury is foreseeable.

	8.
	Maximum height: base ratio not to exceed 3.5:1 (internal) or 3:1 (external) unless ties are used.

	9.
	Men and materials must not be allowed to remain on MSTs whilst they are being moved.

	10.
	Ties are in place as required when the scaffold is erected. These ties are checked regularly.

	11.
	Intermediate platforms have guard rails (or other suitable barriers) in place.

	12.
	Castor wheels are locked off to secure the tower.

	13.
	The manufacturers’ instructions are followed for erection, use and dismantling.

	14.
	Towers are erected vertically and the outriggers/legs rested on firm level ground.

	15.
	Ladders/step ladders are not used on tower scaffolds.

	16.
	Ties are in place when towers are sheeted, likely to be exposed to high winds, used for carrying out grit blasting, shot blasting, if heavy materials are lifted from the ground up the outside of the tower or if the height to base ratio is exceeded.

	
	

	Remember:

Always check in your safety manual for Company safety procedures and systems of work.

Refer to other assessments for activities connected with this assessment.


	RISK ASSESSMENT

Mobile Scaffolding Tower (MST)
	Ref: S003

	
	Page 2 of 2

	ADDITIONAL CONTROL MEASURES: (Review at workplace and add any additional specific controls required)




	PERSONAL PROTECTIVE EQUIPMENT:

The following PPE will be required for the work activities stated. Ensure the correct TYPE of PPE is selected.

	Head Protection
	(
	Eye/Face Protection
	
	Hearing Protection
	
	Hi-visibility Clothing
	(
	Gloves
	(

	Foot Protection
	(
	Safety Clothing
	
	R.P.E.
	
	Fall Arrest Equipment
	(
	
	

	REVIEW AND MONITORING:

Review in light of further information becoming available or a change in conditions/circumstances.



	INFORMATION TO BE PROVIDED TO EMPLOYEES:

Information contained in this assessment.



	The following persons have received the information contained in this assessment:

	Name
	Date
	Initial
	Name
	Date
	Initial

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	SIGNED BY ASSESSOR:
Iain Brook
	DATE:
June 2020

	


	RISK ASSESSMENT

Step Ladders.
	Ref: S014

	
	Page 1 of 2

	EMPLOYER: Harry Brook & Son Ltd

	LOCATION:  NBS 74 king street Manchester M2 4NJ

	ASSESSED BY:   Carl Hudson
	DESIGNATION:    H & S Director

	LEGEND:   Likelihood and Severity:- 1 = Low  2 = Medium  3 = High

   Risk Rating (L x S):-  1-4 = Low (Acceptable)  6 = Medium (Consider further controls)  9 = Unacceptable (Do not proceed)

	SIGNIFICANT HAZARDS IDENTIFIED:

Give a brief description of what could be reasonably expected to cause significant harm and how that harm may arise.
	RISK ASSESSMENT

	
	UNCONTROLLED
	CONTROLLED

	
	L
	S
	RR
	L
	S
	RR

	Falling off step ladder or landing on persons below
	2
	3
	6
	1
	3
	3

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	PERSONS AT RISK
	Y/N
	DETAIL

	EMPLOYEES
	Y
	Operatives

	CONTRACTORS
	Y
	Others working within the vicinity

	MEMBERS OF PUBLIC
	Y
	Persons within the vicinity

	OTHERS
	Y/N
	

	CONTROL MEASURES:

	1.
	Ensure adequate length step ladders are used to prevent standing on the top three rungs.

	2.
	Standing directly onto the top rung is prohibited unless the ladder is designed to do so.

	3.
	Step ladders are used in accordance with manufacturers’ recommendations.

	4.
	All step ladders are in good condition.

	5.
	Step ladder feet will be placed on level and firm footage.

	6.
	Side loading of step ladders is not undertaken.

	7.
	Step ladders are regularly inspected by competent persons.

	8.
	Step ladders are not overloaded and are used for lightweight duty only.

	
	

	
	

	
	

	
	

	
	

	
	

	
	

	
	

	
	

	
	

	
	

	
	

	
	

	Remember:

Always check in your safety manual for Company safety procedures and systems of work.

Refer to other assessments for activities connected with this assessment.


	RISK ASSESSMENT

Step Ladders
	Ref: S014

	
	Page 2 of 2

	ADDITIONAL CONTROL MEASURES: (Review at workplace and add any additional specific controls required)




	PERSONAL PROTECTIVE EQUIPMENT:

The following PPE will be required for the work activities stated. Ensure the correct TYPE of PPE is selected.

	Head Protection
	(
	Eye/Face Protection
	
	Hearing Protection
	
	Hi-visibility Clothing
	(
	Gloves
	

	Foot Protection
	(
	Safety Clothing
	
	R.P.E.
	
	Fall Arrest (in MEWP)
	
	
	

	REVIEW AND MONITORING:

Review in light of further information becoming available or a change in conditions/circumstances.



	INFORMATION TO BE PROVIDED TO EMPLOYEES:

Information contained in this assessment.



	The following persons have received the information contained in this assessment:

	Name
	Date
	Initial
	Name
	Date
	Initial

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	SIGNED BY ASSESSOR:
Iain Brook
	DATE:

June 2020

	


	RISK ASSESSMENT

Work At Height
	Ref: W003

	
	Page 1 of 2

	EMPLOYER:     Harry Brook & Son Limited

	LOCATION      NBS 74 king street Manchester M2 4NJ

	ASSESSED BY:   Carl Hudson
	DESIGNATION:    H & S Director

	LEGEND:   Likelihood and Severity:- 1 = Low  2 = Medium  3 = High

   Risk Rating (L x S):-  1-4 = Low (Acceptable)  6 = Medium (Consider further controls)  9 = Unacceptable (Do not proceed)

	SIGNIFICANT HAZARDS IDENTIFIED:

Give a brief description of what could be reasonably expected to cause significant harm and how that harm may arise.
	RISK ASSESSMENT

	
	UNCONTROLLED
	CONTROLLED

	
	L
	S
	RR
	L
	S
	RR

	Falls of persons from working place or accesses
	3
	3
	9
	1
	3
	3

	Falls of materials or articles
	3
	3
	9
	1
	3
	3

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	PERSONS AT RISK
	Y/N
	DETAIL

	EMPLOYEES
	Y
	Operatives undertaking the activity

	CONTRACTORS
	Y
	Persons within the vicinity

	MEMBERS OF PUBLIC
	Y/N
	

	OTHERS
	Y/N
	

	CONTROL MEASURES:

	1.
	Ensure work is carried out as planned and in accordance with the relevant standards and risk assessments, also that operatives have received instructions in safe working procedures and the use of any safety equipment provided.

	2..
	Ensure operatives inspect safety equipment weekly and prior to use, any defective equipment to be exchanged or repaired before use. 

	3.
	All necessary precautions are taken to ensure that persons do not walk or work beneath operatives carrying out work at high level.

	4.
	All operatives working at height must wear the appropriate personal protective equipment., i.e. safety belts, harnesses, fall arrest devices, etc.

	5.
	The safety of other workers, the public and particularly children must be a priority consideration during the working period. Access to working areas must be removed or fenced outside working hours or when unattended.

	6.
	All work at height areas will be guarded to prevent falls of persons and materials where practicable, or other suitable protective procedures will be used.

	7.
	Control measures identified must also be implemented.

	
	

	
	

	
	

	
	

	
	

	
	

	
	

	
	

	Remember:

Always check in your safety manual for Company safety procedures and systems of work.

Refer to other assessments for activities connected with this assessment.
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	ADDITIONAL CONTROL MEASURES: (Review at workplace and add any additional specific controls required)




	PERSONAL PROTECTIVE EQUIPMENT:

The following PPE will be required for the work activities stated. Ensure the correct TYPE of PPE is selected.

	Head Protection
	(
	Eye/Face Protection
	
	Hearing Protection
	
	Hi-visibility Clothing
	(
	Gloves
	

	Foot Protection
	(
	Safety Clothing
	
	R.P.E.
	
	Fall Arrest (in MEWP)
	(
	
	

	REVIEW AND MONITORING:

Review in light of further information becoming available or a change in conditions/circumstances.



	INFORMATION TO BE PROVIDED TO EMPLOYEES:

Information contained in this assessment.

Site safety induction.

Information contained in method statement (if applicable).



	The following persons have received the information contained in this assessment:

	Name
	Date
	Initial
	Name
	Date
	Initial
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Iain Brook
	DATE:

June 2020

	


Harry Brook & Son Limited – Risk Assessments – Revision 01


