Supporting Information for Discharge of Planning Conditions
Project: Vaughan Street Industrial Estate Padel Centre
Planning Reference: 141847/FO/2025
1. EV Charger Specification (Condition no. 3)
Proposed EV Charger Specification:
- Type: Fast AC Electric Vehicle Charger
- Power Output: Minimum 7.2kW (Single-Phase AC)
- Connector Type: Universal Type 2 Socket
- Mounting: Wall-Mounted 
- Finish: Compact grey casing, weather-resistant (IP66)
- Example Model: EO Mini Pro 3

Cable routing to the EV charger will be provided via surface-mounted conduit along the wall or via buried ducting, depending on final site conditions. The final installed unit will comply with the IET Code of Practice for Electric Vehicle Charging Equipment Installation.
2. Planter Details (Condition no. 8)
Planters will be positioned at the front entrance of the building.
- Area Available: Approx. 3m wide x 1m deep
- Planter Type: Square/Rectangular pots
- Approximate Number: 3–4 planters depending on final sizing
- Planting: Low-maintenance shrubs and seasonal flowers (final species to be selected closer to installation).
3. Bin Store and Waste Management Notes (Condition no. 6)
Bin storage will be located near the front entrance on the left-hand side.
- Bin Types and Quantities:
  1 x 1100L General Waste Bin
  1 x 1100L Mixed Recycling Bin
  1 x 240L Food Waste Bin
- Collection Frequency: Weekly
Refuse vehicle access to the bin store area is available via the main site access route. Basic refuse tracking lines will be shown on the submitted external plan.
Mixed recycling and general waste bins will be provided around the premises. Will be collected and emptied on daily basis (more if required) and deposited into the external storage bins.
A Waste Proforma Form will accompany this submission confirming the above storage capacity and collection frequency.
4. Cycle Parking Details (Condition no. 5) 
Cycle storage will be located near the front entrance on the right-hand side of the building.
- Capacity: 4 cycles
- Shelter Type: Open-sided shelter with roof..
- Fixings: Secure fixing hoops (Sheffield stands) to allow cycles to be locked in place.
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