63-65 Upper Chorlton Road, Manchester
Approval Ref: 141366/JO/2024 (formerly 138589/FO/2023) 
Covering Note Relating to Application to Discharge Condition 23 – Recessing of brickwork to sealed windows

Overview
Condition 23 relates to 2no. small existing windows on the north elevation of the original outrigger.  These are to be sealed with recessed brickwork so as to minimise the risk of fire spread between flats.  We can confirm that the new brickwork in question will be recessed by 20mm from the face of the existing brickwork
