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	COSHH Assessment for:
	Soudafoam B1
	Ref:
	493

	Assessor:
	Dom Reddall
	Date:
	07.02.23
	Next Review:
	07.02.26

	Describe the activity or work process:

	Soudafoam B1 an all-purpose, handheld gap filling expanding PU Foam

	

	All roof areas.

	Identify the Persons at Risk:
	Employees
	
	Contractors
	
	Public
	

	Name the substance involved in the process, the quantity and its manufacturer.
(A copy of a current safety data sheet for this substance should be attached)

	Soudafoam B1 by Soudal Ltd.

	 Explain why a safer alternative cannot be used:

	Soudafoam B1 is produced for general market and deemed safe to use.

	Classification (tick all that apply):

	Physical Hazards

	Unstable Explosive
	Flammable
	Oxidising
	Compressed Gas
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	

	Health Hazards
	Environmental

	Toxic
	Corrosive
	Irritant
	Resp. Sens/Health
	Environmental
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	

	Hazard Type:

	Gas
	Vapour
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other:

	
	
	
	
	
	
	
	

	Route of Exposure:

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (State)

	
	
	
	
	

	Explosive Limits and Workplace Exposure Limits (WELs) 

	Long-term exposure level (8hrTWA):
	Short-term exposure level (15 mins):

	UEL:   
Diethyl ether – 100 ppm, 310mg/m3

	LEL: 
Diethyl ether – 200ppm, 620mg/m3 


	Detail Potential Health Risks:

	
H222 - Extremely flammable aerosol.
H229 - Pressurised container: May burst if heated.
H315 - Causes skin irritation.
H317 - May cause an allergic skin reaction.
H319 - Causes serious eye irritation.
H332 - Harmful if inhaled.
H334 - May cause allergy or asthma symptoms or breathing difficulties if inhaled.
H335 - May cause respiratory irritation.
H351 - Suspected of causing cancer.
H373 - May cause damage to organs through prolonged or repeated exposure.

	Control & Recovery Measures Actioned: (for example extraction, ventilation, training, supervision).  Include special measures for vulnerable groups, such as disabled people and pregnant workers.  
Take account of those substances that are produced from activities undertaken by another employer’s employees.

	Ventilation:
	Accidental Release & Spillage Plan :

	Ensure good ventilation. In case of inadequate ventilation wear respiratory protection.
	Ventilate spillage area. No open flames, no sparks, and no 
smoking. Do not breathe
dust/fume/gas/mist/vapours/spray. Avoid contact with
skin and eyes.

	Special Transport:
	Signage, provision of information and instruction:

	
	Brief this COSHH

	Fire Precautions/Extinguisher Type:
	Environmental Considerations:

	Fire Precautions /  
Extinguisher Type: Water spray. Dry powder. Foam. Carbon dioxide.
	Avoid release to the environment.

	Storage Required:
	Disposal Issues:

	N/A
	 Hazardous waste

	Is health surveillance or monitoring required for foreseeable exposure potential?

	Routine health screening
	
	Personal air monitoring
	
	Background air monitoring
	

	Personal Protective Equipment (state type and standard)

	Item
	Tick
	Requirement
	Item
	Tick
	Requirement
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	Safety glassess (EN 166)
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	Protective gloves (EN 374)
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	Protective working garments
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	Other
	
	

	First Aid Measures

	First-aid measures after inhalation : Remove person to fresh air and keep comfortable for breathing. Call a poison center or a doctor if you feel unwell.
First-aid measures after skin contact : Wash skin with plenty of water. Take off contaminated clothing. If skin irritation or rash occurs: Get medical advice/attention.
First-aid measures after eye contact : Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing. If eye irritation persists: Get medical advice/attention.
First-aid measures after ingestion : Call a poison center or a doctor if you feel unwell.

	Disposal Instructions for substance and empty containers:

	Hazardous Waste
	
	General Waste
	

	Return to Depot
	
	Return to Supplier
	

	Other/Notes:

	

	Is exposure adequately controlled?
	Yes
	
	No
	

	Risk Rating Following Above Controls:
	High
	
	Med
	  
	Low
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