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	COSHH Assessment for:
	Cortex 0787 Non Flammable Primer
	Ref:
	354

	Assessor:
	Dominic Reddall
	Date:
	September 2022
	Next Review:
	September 2025

	Describe the activity or work process:

	

	What is the location of the activity or work process?

	Site 

	Identify the Persons at Risk:
	Employees
	
	Contractors
	
	Public
	

	Name the substance involved in the process, the quantity and its manufacturer.
(A copy of a current safety data sheet for this substance should be attached)

	Cortex 0787 Non Flammable Primer

	 Explain why a safer alternative cannot be used:

	Substitution is not possible as the substance has been specified by the client

	Classification (tick all that apply):

	Physical Hazards

	Unstable Explosive
	Flammable
	Oxidising
	Compressed Gas
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	

	Health Hazards
	Environmental

	Toxic
	Corrosive
	Irritant
	Resp. Sens/Health
	Environmental
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	

	Hazard Type:

	Gas
	Vapour
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other:

	
	
	
	
	
	
	
	Absorption

	Route of Exposure:

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (State)

	
	
	
	
	

	Explosive Limits and Workplace Exposure Limits (WELs) 

	Long-term exposure level (8hrTWA):
	Short-term exposure level (15 mins):

	WEL 100 ppm(Sk) 350 mg/ m3(Sk)
	WEL 300 ppm(Sk) 1060 mg/m3(Sk)

	Detail Potential Health Risks:

	
Inhalation: Vapours may cause drowsiness and dizziness. 
Irritation of nose, throat and airway.
Ingestion: May cause chemical burns in mouth and throat.
Skin contact: Prolonged skin contact may cause redness and irritation.
Eye contact: Severe irritation, burning and tearing.


	Control & Recovery Measures Actioned: (for example extraction, ventilation, training, supervision).  Include special measures for vulnerable groups, such as disabled people and pregnant workers.  
Take account of those substances that are produced from activities undertaken by another employer’s employees.

	Ventilation:
	Accidental Release & Spillage Plan :

	Provide adequate ventilation. Avoid inhalation of vapours. Observe any occupational exposure limits for the product or ingredients.
	Prevent spillage into watercourses and sewers.

	Special Transport:
	Signage, provision of information and instruction:

	UN No. (ADR/RID): 2810
UN No. (IMDG): 2810
UN No. (ICAO): 2810
UN No. (ADN): 2810
	Brief of this assessment.

	Fire Precautions/Extinguisher Type:
	Environmental Considerations:

	Extinguish with foam, carbon dioxide, dry
powder or water fog.
	Environmental precautions: Do not discharge into drains or watercourses or onto the ground.

	Storage Required:
	Disposal Issues:

	Keep away from heat, sparks and open flame. Store
in closed original container at temperatures between 5°C and 25°C.
	Waste should be treated as controlled waste. Dispose
of waste to licensed waste disposal site in accordance with the
requirements of the local Waste Disposal Authority.

	Is health surveillance or monitoring required for foreseeable exposure potential?

	Routine health screening
	No
	Personal air monitoring
	No
	Background air monitoring
	No

	Personal Protective Equipment (state type and standard)

	Item
	Tick
	Requirement
	Item
	Tick
	Requirement
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	Chemical
splash goggles or face shield.
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	If ventilation is inadequate, suitable respiratory
protection must be worn. In confined or poorly- ventilated spaces, a
supplied-air respirator must be worn. Wear a respirator fitted with the
following cartridge: Particulate filter, type P3. ABEK2-P3: Environmental
exposure controls
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	Chemical
splash goggles or face shield.
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	It is recommended that gloves are made of the following
material: Nitrile rubber. It should be noted that liquid may penetrate the
gloves. Frequent changes are recommended. For exposure up to 8 hours,
wear gloves made of the following material: Viton rubber (fluoro rubber).
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	Wear suitable protective clothing as
protection against splashing or contamination. Wear apron or protective clothing in case of contact.
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	Other
	
	

	First Aid Measures

	Remove affected person from source of contamination.
Inhalation: Move affected person to fresh air at once.
Ingestion: DO NOT induce vomiting. Get medical attention immediately.
Skin contact: Remove contaminated clothing immediately and wash skin
with soap and water.
Eye contact: Rinse immediately with plenty of water. Remove any contact
lenses and open eyelids wide apart. Continue to rinse for at least 15
minutes. Get medical attention if irritation persists after washing. Show
this Safety Data Sheet to the medical personnel.
Inhalation: Vapours may cause drowsiness and dizziness. 
Irritation of nose, throat and airway.
Ingestion: May cause chemical burns in mouth and throat.
Skin contact: Prolonged skin contact may cause redness and irritation.
Eye contact: Severe irritation, burning and tearing


	Disposal Instructions for substance and empty containers:

	Hazardous Waste
	
	General Waste
	

	Return to Depot
	
	Return to Supplier
	

	Other/Notes:

	Dispose of as hazardous waste in compliance with local and national regulations. Where possible recycling is preferred to disposal or incineration.


	Is exposure adequately controlled?
	Yes
	
	No
	

	Risk Rating Following Above Controls:
	High
	
	Med
	
	Low
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