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	COSHH Assessment for:
	Lead Metal
	Ref:
	445

	Assessor:
	Dominic Reddall
	Date:
	May 2022
	Next Review:
	May 2025

	Describe the activity or work process:

	Lead tiles used as a roofing application.

	What is the location of the activity or work process?

	Various roof areas as per client specification.

	Identify the Persons at Risk:
	Employees
	
	Contractors
	
	Public
	

	Name the substance involved in the process, the quantity and its manufacturer.
(A copy of a current safety data sheet for this substance should be attached)

	Lead in a solid state available from various manufacturers.
The quantity to be used will depend on job specification although the minimum amount of lead possible will be used for all tasks.

	 Explain why a safer alternative cannot be used:

	Specified by the client.

	Classification (tick all that apply):

	Physical Hazards

	Unstable Explosive
	Flammable
	Oxidising
	Compressed Gas
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	

	Health Hazards
	Environmental

	Toxic
	Corrosive
	Irritant
	Resp. Sens/Health
	Environmental
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	

	Hazard Type:

	Gas
	Vapour
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other:

	
	
	
	
	
	
	
	

	Route of Exposure:

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (State)

	
	
	
	
	

	Explosive Limits and Workplace Exposure Limits (WELs) 

	Long-term exposure level (8hrTWA):
	Short-term exposure level (15 mins):

	UEL: N/A in sold state
	LEL: N/A in solid state

	Detail Potential Health Risks:

	Used in its solid state lead poses minimal hazard.
Lead is a very heavy metal therefore manual handling tasks involving lead should be assessed and planned carefully.
Ingestion of lead through contact with contaminated fingers etc. is unlikely to cause immediate adverse symptoms although prolonged or significant exposure can lead to a build up of lead in the body causing lead poisoning.

	Control & Recovery Measures Actioned: (for example extraction, ventilation, training, supervision).  Include special measures for vulnerable groups, such as disabled people and pregnant workers.  
Take account of those substances that are produced from activities undertaken by another employer’s employees.

	Ventilation:
	Accidental Release & Spillage Plan :

	N/a in solid state and only cut with hand tools.
	N/a in solid state and only cut with hand tools.

	Special Transport:
	Signage, provision of information and instruction :

	Handle with extereme care as lead is very heavy.
	Briefing of this assessment.

	Fire Precautions/Extinguisher Type:
	Environmental Considerations :

	Extinguisher Type: Non flammable although lead will melt and release toxic fumes. Molten led could ignite other substances.
	Do not disperse lead compounds in the atmosphere or allow to enter drains and river

	Storage Required:
	Disposal Issues:

	No special requirements
	Recycle if possible. Hazardous waste if disposed of.

	Is health surveillance or monitoring required for foreseeable exposure potential?

	Routine health screening
	No
	Personal air monitoring
	No
	Background air monitoring
	No

	Personal Protective Equipment (state type and standard)

	Item
	Tick
	Requirement
	Item
	Tick
	Requirement
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	Not in solid state using only hand tools
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	Not in solid state using only hand tools
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	Wear chemical resistant gloves in cases of prolonged or repeated contact
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	Issued uniform
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	Safety footwear (EN345 SB Compliant) due to weight of the metal. BS EN 345 compliant

	Other
	
	

	First Aid Measures

	INHALATION: Move exposed person to fresh air at once. Get medical attention promptly.
INGESTION: Do not induce vomiting. If person is conscious, rinse mouth thoroughly and encourage the drinking of large quantity of water. Get medical attention immediately.
SKIN CONTACT: Remove all contaminated clothing and footwear immediately, unless it is stuck to the skin.
Wash the affected skin immediately with soap and water. Get medical attention if irritation
persists.
EYE CONTACT: Make sure that any contact lenses are removed from the eyes before rinsing. Promptly
wash eyes with plenty of water while lifting the eyelids. Get medical attention immediately.

	Disposal Instructions for substance and empty containers:

	Hazardous Waste
	
	General Waste
	

	Return to Depot
	
	Return to Supplier
	

	Other/Notes:

	

	Is exposure adequately controlled?
	Yes
	
	No
	

	Risk Rating Following Above Controls:
	High
	
	Med
	
	Low
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