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	COSHH Assessment for:
	Flexcrete Monolite
	Ref:
	480

	Assessor:
	Dom Reddall
	Date:
	16/11/22
	Next Review:
	16/11/25

	Describe the activity or work process:

	Monolite is used for concrete repairs.

	

	On site

	Identify the Persons at Risk:
	Employees
	
	Contractors
	`
	Public
	

	Name the substance involved in the process, the quantity and its manufacturer.
(A copy of a current safety data sheet for this substance should be attached)

	Monolite by Flexcrete Technologies Ltd.

	 Explain why a safer alternative cannot be used:

	N/A

	Classification (tick all that apply):

	Physical Hazards

	Unstable Explosive
	Flammable
	Oxidising
	Compressed Gas
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	

	Health Hazards
	Environmental

	Toxic
	Corrosive
	Irritant
	Resp. Sens/Health
	Environmental
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	

	Hazard Type:

	Gas
	Vapour
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other:

	
	
	
	
	
	
	
	

	Route of Exposure:

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (State)

	
	
	
	
	

	Explosive Limits and Workplace Exposure Limits (WELs) 

	Long-term exposure level (8hrTWA):
	Short-term exposure level (15 mins):

	UEL:   
	LEL: 

	Detail Potential Health Risks:

	Hazard statements
H318: Causes serious eye damage
H315: Causes skin irritation
H317: May cause an allergic skin reaction
H335: May cause respiratory irritation






	Control & Recovery Measures Actioned: (for example extraction, ventilation, training, supervision).  Include special measures for vulnerable groups, such as disabled people and pregnant workers.  
Take account of those substances that are produced from activities undertaken by another employer’s employees.

	Ventilation:
	Accidental Release & Spillage Plan :

	Ensure good ventilation in the workplace. Prevent formation of dust.
	Move containers from spill area. Avoid dust 
generation. Using a vacuum with HEPA filter will 
reduce dust dispersal. Place spilled material in a 
designated, labelled waste container. Dispose of via a licensed waste disposal contractor.

	Special Transport:
	Signage, provision of information and instruction:

	
	Briefiing of this COSHH Asessment

	Fire Precautions/Extinguisher Type:
	Environmental Considerations:

	Fire Precautions /  
Extinguisher Type: 
	Avoid dispersal of spilt material and runoff and contact with soil, waterways, drains 
and sewers. Inform the relevant authorities if the product has caused environmental 
pollution (sewers, waterways, soil or air).

	Storage Required:
	Disposal Issues:

	N/A
	 

	Is health surveillance or monitoring required for foreseeable exposure potential?

	Routine health screening
	
	Personal air monitoring
	
	Background air monitoring
	

	Personal Protective Equipment (state type and standard)

	Item
	Tick
	Requirement
	Item
	Tick
	Requirement
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	Appropriate respirator FFP3
If there is a risk of exceeding the exposure limits,
e. g. the open fiddling with the powdered dry product or during
processing by splash, an appropriate respirator must be used.
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	Wear approved glasses or goggles according to EN 166 
with anti-mist for eye protection when handling wet or dry 
material
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	EN374 -chemical resistant gloves
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	Wear protective long-sleeved clothing and tight shoes. EN ISO 13688
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	Other
	
	

	First Aid Measures

	Inhalation - Remove to fresh air. Keep person warm and at rest. If not breathing, if breathing is irregular or if respiratory arrest occurs, provide artificial respiration or oxygen by trained personnel. Seek medical attention.
Eye Contact - Check for and remove any contact lenses. Immediately flush eyes with running 
water for at least 15 minutes, keeping eyelids open. Seek immediate medical 
attention.
Skin Contact - Remove contaminated clothing and shoes. Wash skin thoroughly with soap and 
water or use recognised skin cleanser. Seek medical attention if irritation persists.
Do NOT use solvents or thinners
Ingestion - If swallowed, seek medical advice immediately and show the container or label. Keep person warm and at rest. Do NOT induce vomiting.



	Disposal Instructions for substance and empty containers:

	Hazardous Waste
	
	General Waste
	

	Return to Depot
	
	Return to Supplier
	

	Other/Notes:

	

	Is exposure adequately controlled?
	Yes
	
	No
	

	Risk Rating Following Above Controls:
	High
	
	Med
	  
	Low
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