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	COSHH Assessment for:
	Siderise Stonewool
	Ref:
	358

	Assessor:
	Dominic Reddall
	Date:
	April 2022
	Next Review:
	April 2025

	Describe the activity or work process:

	Fire, acoustic and thermal insulation.

	What is the location of the activity or work process?

	Site 

	Identify the Persons at Risk:
	Employees
	
	Contractors
	
	Public
	

	Name the substance involved in the process, the quantity and its manufacturer.
(A copy of a current safety data sheet for this substance should be attached)

	Siderise Stonewool

	 Explain why a safer alternative cannot be used:

	Substitution is not possible as the substance has been specified by the client

	Classification (tick all that apply):

	Physical Hazards

	Unstable Explosive
	Flammable
	Oxidising
	Compressed Gas
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	

	Health Hazards
	Environmental

	Toxic
	Corrosive
	Irritant
	Resp. Sens/Health
	Environmental
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	

	Hazard Type:

	Gas
	Vapour
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other:

	
	
	
	
	
	
	
	

	Route of Exposure:

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (State)

	
	
	
	
	

	Explosive Limits and Workplace Exposure Limits (WELs) 

	Long-term exposure level (8hrTWA):
	Short-term exposure level (15 mins):

	Workplace exposure limit (WEL) 5mg/m3 gravimetric measure (total inhalable dust) and 2 fibres/ml
airborne fibre limit, 8-hour time weighted averages.
	N/A

	Detail Potential Health Risks:

	
The overall conclusion in accordance with the REACH regulation is that there are no hazardous
classifications associated with stone wool fibres in respect to physical, health and environmental
considerations.



	Control & Recovery Measures Actioned: (for example extraction, ventilation, training, supervision).  Include special measures for vulnerable groups, such as disabled people and pregnant workers.  
Take account of those substances that are produced from activities undertaken by another employer’s employees.

	Ventilation:
	Accidental Release & Spillage Plan :

	General ventilation is recommended.
	N/A

	Special Transport:
	Signage, provision of information and instruction:

	N/A

	Brief of this assessment.

	Fire Precautions/Extinguisher Type:
	Environmental Considerations:

	Water, foam, carbon dioxide or dry powder.
	None required.

	Storage Required:
	Disposal Issues:

	Keep material in original packaging until it is to be used. Store material to protect against damage
including the weather.
	Spray with water before sweeping or use vacuum equipment.

	Is health surveillance or monitoring required for foreseeable exposure potential?

	Routine health screening
	No
	Personal air monitoring
	No
	Background air monitoring
	No

	Personal Protective Equipment (state type and standard)

	Item
	Tick
	Requirement
	Item
	Tick
	Requirement
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	If the WEL is likely to be exceeded (for example when using high speed cutting tools or when
working in confined spaces) disposable face masks complying with BS EN149 FFP1 or FFP2 should
be used and are suitable for most applications.
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	Use of safety goggles to EN166 is advised.
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	It is recommended that gloves in conformity with EN 388
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	Other
	
	

	First Aid Measures

	In case of discomfort, leave dusty area. Blow nose and rinse throat with clean water to clear any dust.
In case of discomfort, remove contaminated clothing and wash skin gently with clean cold water
and mild soap.
In case of contact with eyes, rinse abundantly with clean water for at least 15 minutes.
If ingested, drink plenty of water.
The mechanical effect of fibres in contact with skin can cause temporary itching.

	Disposal Instructions for substance and empty containers:

	Hazardous Waste
	
	General Waste
	

	Return to Depot
	
	Return to Supplier
	

	Other/Notes:

	SIDERISE stone wool material is recyclable. Stone wool insulation is classified as non-hazardous waste. stone wool insulation waste is covered by the non-hazardous entry “17 06 04 insulation materials other than those mentioned in 17 06 01 and 17 06 03” in the European Waste Catalogue, established by EC Decision 2000/532/EC (hazardous waste). 

Under landfill regulations SIDERISE
insulation waste is categorised as “waste accepted at landfills for non-hazardous waste” in
accordance with EC Decision 2003/33/ EC.

	Is exposure adequately controlled?
	Yes
	
	No
	

	Risk Rating Following Above Controls:
	High
	
	Med
	
	Low
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