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	COSHH Assessment for:
	Cortex 0771FR Paste Adhesive
	Ref:
	352

	Assessor:
	Dominic Reddall
	Date:
	April 2022
	Next Review:
	April 2025

	Describe the activity or work process:

	Joint sealant. Can be used in applications which require sealants of fire-retardant properties

	What is the location of the activity or work process?

	Site 

	Identify the Persons at Risk:
	Employees
	
	Contractors
	
	Public
	

	Name the substance involved in the process, the quantity and its manufacturer.
(A copy of a current safety data sheet for this substance should be attached)

	Cortex 0771FR Paste Adhesive, Cortex, Quantity depending on customer requirements.

	 Explain why a safer alternative cannot be used:

	Substitution is not possible as the substance has been specified by the client

	Classification (tick all that apply):

	Physical Hazards

	Unstable Explosive
	Flammable
	Oxidising
	Compressed Gas
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	

	Health Hazards
	Environmental

	Toxic
	Corrosive
	Irritant
	Resp. Sens/Health
	Environmental
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	

	Hazard Type:

	Gas
	Vapour
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other:

	
	
	
	
	
	
	
	

	Route of Exposure:

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (State)

	
	
	
	
	

	Explosive Limits and Workplace Exposure Limits (WELs) 

	Long-term exposure level (8hrTWA):
	Short-term exposure level (15 mins):

	TWA (8 Hour) 200ppm
260mg/m3
	N/A

	Detail Potential Health Risks:

	
Respiratory or skin sensitisation.









	Control & Recovery Measures Actioned: (for example extraction, ventilation, training, supervision).  Include special measures for vulnerable groups, such as disabled people and pregnant workers.  
Take account of those substances that are produced from activities undertaken by another employer’s employees.

	Ventilation:
	Accidental Release & Spillage Plan :

	In case of insufficient ventilation, wear suitable respiratory equipment. Make sure there is good local exhaust ventilation during hot air welding.
	Personal precautions: Use personal protective equipment. Deny access to
unprotected persons.

	Special Transport:
	Signage, provision of information and instruction:

	Not classified as hazardous for transport according to national and international transport regulations.
	Brief of this assessment.

	Fire Precautions/Extinguisher Type:
	Environmental Considerations:

	Suitable Fire Fighting medium Water/CO2/Sand/Foam
	If the product contaminates rivers and lakes
or drains inform respective authorities.
No special environmental precautions required.

	Storage Required:
	Disposal Issues:

	Keep container tightly closed in a dry and well-ventilated place. Store in accordance with local regulations.
	Dispose of surplus and non-recyclable products via a licensed waste disposal contractor.


	Is health surveillance or monitoring required for foreseeable exposure potential?

	Routine health screening
	No
	Personal air monitoring
	No
	Background air monitoring
	No

	Personal Protective Equipment (state type and standard)

	Item
	Tick
	Requirement
	Item
	Tick
	Requirement
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In case of inadequate ventilation wear respiratory protection.

Respirator selection must be based on known or anticipated exposure
levels, the hazards of the product and the safe work-ing limits of the
selected respirator.

Organic vapour filter (Type A)
A1: < 1000 ppm; A2: < 5000 ppm; A3: < 10000 ppm
Ensure adequate ventilation. This can be achieved by local exhaust
extraction or by general ventilation.
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Safety glasses with side-shields conforming to EN166
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Chemical-resistant, impervious gloves complying with
an approved standard must be worn at all times when handling chemical
products. Reference number EN 374. Follow manufacturer specifications.
Suitable for short time use or protection against splashes: Butyl rubber/
nitrile rubber gloves (0,4 mm)
Contaminated gloves should be removed.
Suitable for permanent exposure:
Viton gloves (0.4 mm), breakthrough time >30 min.
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Protective clothing 
Long-sleeved working clothing, long trousers). Rubber aprons and protective boots are additionally recommended for mixing
and stirring work.
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	Safety shoes acc. to
EN ISO 20345,
	Other
	
	

	First Aid Measures

	If inhaled:
Move to fresh air.
Consult a physician after significant exposure.

In case of skin contact:
Take off contaminated clothing and shoes immediately.
Wash off with soap and plenty of water.
If symptoms persist, call a physician.

In case of eye contact:
Immediately flush eye(s) with plenty of water.
Remove contact lenses.
Keep eye wide open while rinsing.
If eye irritation persists, consult a specialist.

If swallowed:
Do not induce vomiting without medical advice.
Rinse mouth with water.
Do not give milk or alcoholic beverages.
Never give anything by mouth to an unconscious person.


	Disposal Instructions for substance and empty containers:

	Hazardous Waste
	
	General Waste
	

	Return to Depot
	
	Return to Supplier
	

	Other/Notes:

	
The generation of waste should be avoided or minimized
wherever possible. Empty containers or liners may retain some product residues. This
material and its container must be disposed of in a safe way.

Dispose of surplus and non-recyclable products via a licensed waste
disposal contractor.

Disposal of this product, solutions and any by-products should at all times
comply with the requirements of environmental protection and waste
disposal legislation and any regional local authority requirements.

Avoid dispersal of spilled material and runoff and contact with soil,
waterways, drains and sewers.


	Is exposure adequately controlled?
	Yes
	
	No
	

	Risk Rating Following Above Controls:
	High
	
	Med
	
	Low
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