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Description automatically generated]Applying Water Job Card

BUILD NAME: __________________________             		DATE:             _____________
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Description automatically generated]Ice Applying Water Job Card

BUILD NAME: __________________________             		DATE:             _____________

Tooling / Equipment

Safety Notes
Whilst the pipes are freezing there is to be NO foot traffic across the pipe mats unless it is an ice crew or chiller supplier.

	No.
	[bookmark: _Hlk131589485]TASK 1 – Set Chiller and apply water for freezing.
	tICK
(when completed)

	1
	The chiller system will now have a set point of -12°c and the pipes will begin to freeze.
	

	2
	Now you can start to fill the rink with water. Once the water has reached halfway above the aluminum pipes, it would be time to complete the commissioning sheet and handover to the customer.
	

	3
	Continue to monitor for leaks, check rink mat pressures, ensure the chillers and pumps are working and are at temperatures set as per commissioning sheet.
	

	4
	If any issues identified refer to commissioning sheet.
	

	
	[bookmark: _Hlk131590212]SIGNATURE
	DATE

	
	
	



Refer to Ice applying water job card document SYS038-I05 for the next stage.
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