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	COSHH Assessment for:
	Rockwool Insulation
	Ref:
	300

	Assessor:
	Dominic Reddall
	Date:
	April 2022
	Next Review:
	April 2025

	Describe the activity or work process:

	Rockwool Insulation is used as Thermal Insulation, acoustic insulation and fire protection in building construction applications. 

	What is the location of the activity or work process?

	All areas specified by client including cavities, walls, roofs etc 

	Identify the Persons at Risk:
	Employees
	
	Contractors
	
	Public
	

	Name the substance involved in the process, the quantity and its manufacturer.
(A copy of a current safety data sheet for this substance should be attached)

	Quantities will vary dependant on the roof area & job specification.


	 Explain why a safer alternative cannot be used:

	The material and quantity has been specified by the client.	

	Classification (tick all that apply):

	Physical Hazards

	Unstable Explosive
	Flammable
	Oxidising
	Compressed Gas
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	

	Health Hazards
	Environmental

	Toxic
	Corrosive
	Irritant
	Resp. Sens/Health
	Environmental
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	

	Hazard Type:

	Gas
	Vapour
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other:

	
	
	
	
	
	
	
	

	Route of Exposure:

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (State)

	
	
	
	
	

	Explosive Limits and Workplace Exposure Limits (WELs) 

	Long-term exposure level (8hrTWA):
	Short-term exposure level (15 mins):

	Workplace exposure limit (WEL) 5mg/m3 gravimetric
measure (total inhalable dust) and 2 fibres/ml airborne
fibre limit, 8-hour time weighted averages. HSE guidance
assumes that the gravimetric measure would be reached
before the fibre measure. (Ref. HSE EH40).
	















	Detail Potential Health Risks:

	Use of high speed cutting tools can generate dust. The mechanical effect of coarse fibres in contact with
throat, skin or eyes may cause temporary itching/inconvenience.







	Control & Recovery Measures Actioned: (for example extraction, ventilation, training, supervision).  Include special measures for vulnerable groups, such as disabled people and pregnant workers.  
Take account of those substances that are produced from activities undertaken by another employer’s employees.

	Ventilation:
	Accidental Release & Spillage Plan :

	No Specific measures. 
	Vacuum cleaner or dampen with water spray prior to
sweeping up.

	Special Transport:
	Signage, provision of information and instruction :

	N/A
	Breifing this assessment 

	Fire Precautions/Extinguisher Type:
	Environmental Considerations :

	Suitable extinguishing media:
Water, foam, carbon dioxide (CO2), and dry powder
Unsuitable extinguishing media:
None
	None required.

	Storage Required:
	Disposal Issues:

	No Specific measures. 
	Rockwool is recyclable.

	Is health surveillance or monitoring required for foreseeable exposure potential?

	Routine health screening
	No
	Personal air monitoring
	No
	Background air monitoring
	No

	Personal Protective Equipment (state type and standard)

	Item
	Tick
	Requirement
	Item
	Tick
	Requirement
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	When working in unventilated areas or during operations which can generate emission of (various) dusts, wearing a
disposable face mask in accordance with EN 149 FFP1 is recommended.
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	Wear goggles if working above shoulders or where there is heavy dust development. Eye protection to EN 166 is advised.
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	Use gloves conforming with EN 388 to avoid itching.
	[image: ]
	
	Cover exposed skin.
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	Other
	
	

	First Aid Measures

	Inhalation:
Remove from exposure. Rinse the throat and clear dust
from airways.
Skin:
If itching occurs, remove contaminated clothing and wash
skin gently with cold water and mild soap.
Eye:
Rinse abundantly with water for at least 15 minutes.
Ingestion:
Drink plenty of water if accidentally ingested.

	Disposal Instructions for substance and empty containers:

	Hazardous Waste
	
	General Waste
	

	Return to Depot
	
	Return to Supplier
	

	Other/Notes:

	

	Is exposure adequately controlled?
	Yes
	
	No
	

	Risk Rating Following Above Controls:
	High
	
	Med
	
	Low
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