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	COSHH Assessment for:
	HVO Renewable Diesel
	Ref:
	435

	Assessor:
	Dominic Reddall
	Date:
	May 2022
	Next Review:
	May 2025

	Describe the activity or work process:

	Renewable Diesel fuel is used to power various vehicles and large items of plant. This assessment covers general handling, transportation and refuelling processes and should be read in conjunction with the equipment manufacturer’s instructions.

	What is the location of the activity or work process?

	Various site locations as per client specification and project plan.

	Identify the Persons at Risk:
	Employees
	
	Contractors
	
	Public
	

	Name the substance involved in the process, the quantity and its manufacturer.
(A copy of a current safety data sheet for this substance should be attached)

	Diesel from Prema Energy. The quantities to be used will be dependent on how long the equipment must be operated for. The smallest possible quantities will be transported to site and used.

	Explain why a safer alternative cannot be used:

	Equipment is designed to operate on diesel fuel therefore it cannot be substituted.

	Classification (tick all that apply):

	Physical Hazards

	Unstable Explosive
	Flammable
	Oxidising
	Compressed Gas
	

	[image: ]
	[image: ]
	[image: ]
	[image: ]
	

	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	

	Health Hazards
	Environmental

	Toxic
	Corrosive
	Irritant
	Resp. Sens/Health
	Environmental
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	

	Hazard Type:

	Gas
	Vapour
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other:

	
	
	
	
	
	
	
	

	Route of Exposure:

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (State)

	
	
	
	
	

	Explosive Limits and Workplace Exposure Limits (WELs) 

	Long-term exposure level (8hrTWA):
	Short-term exposure level (15 mins):

	
	

	Detail Potential Health Risks:

	May be fatal if swallowed and enters airways.
Repeated exposure may cause skin dryness or cracking.

	Control & Recovery Measures Actioned: (for example extraction, ventilation, training, supervision).  Include special measures for vulnerable groups, such as disabled people and pregnant workers.  
Take account of those substances that are produced from activities undertaken by another employer’s employees.

	Ventilation:
	Accidental Release & Spillage Plan :

	Activities generally take place outdoors. Further assessment required for indoor activities.
	All tanks to be bunded with drip trays at refuelling points. Clear up spills using absorbant material and dispose of as hazardous waste.

	Special Transport:
	Signage, provision of information and instruction :

	
	

	Fire Precautions/Extinguisher Type:
	Environmental Considerations :

	Dry powder, carbon dioxide. Sand. Heavy foam and water fog for professional fire-fighters.
	

	Storage Required:
	Disposal Issues:

	In a tank or a store suitable for combustible liquids. Take precautionary measures to prevent product spills into 
drains, the ground or waters. Take precautions against leakage by constructing collecting pools and sewerage 
systems as well as by surfacing the loading and unloading stations. Retail batches are stored in tightly sealed, 
labelled containers which are impermeable to the product. 
	Empty containers may contain combustible product residues. Empty containers should be taken for local 
recycling or waste disposal

	Is health surveillance or monitoring required for foreseeable exposure potential?

	Routine health screening
	No
	Personal air monitoring
	No
	Background air monitoring
	No

	Personal Protective Equipment (state type and standard)

	Item
	Tick
	Requirement
	Item
	Tick
	Requirement
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	Not required for routine refuelling operations in outdoor or well ventilated areas.
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	Not generally required for routine refuelling operations.
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	Nitrile gloves to prevent skin contact.
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	Issued workwear, long sleeve to prevent splashes onto skin.
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	Other
	
	

	First Aid Measures

	Inhalation: Inhalation is unlikely because of the low vapour pressure of the substance at ambient temperature. If breathed in, move person into fresh air. Consult a physician.
Skin contact: Wash off immediately with soap and plenty of water while removing all contaminated clothes and shoes. If skin irritation persists, call a physician.
Eye contact: Rinse immediately with plenty of water, also under the eyelids. If eye irritation persists, consult a specialist.
Ingestion: DO NOT INDUCE VOMITING. In case of ingestion, always assume that aspiration has occurred. Consult a physician (risk of aspiration into the lungs especially if nausea or irritation occurs)

	Disposal Instructions for substance and empty containers:

	Hazardous Waste
	
	General Waste
	

	Return to Depot
	
	Return to Supplier
	

	Other/Notes:

	Empty containers should be taken for local recycling or waste disposal

	Is exposure adequately controlled?
	Yes
	
	No
	

	Risk Rating Following Above Controls:
	High
	
	Med
	
	Low
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