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	COSHH Assessment for:
	 Rockwool Acoustic Intumescent Sealant 
	Ref:
	301

	Assessor:
	Dominic Reddall 
	Date:
	May 2022
	Next Review:
	May 2025

	Describe the activity or work process:

	Rockwool Acoustic Intumescent Sealant is used to seal joints and service gaps in compartment walls and penetration seals.

	What is the location of the activity or work process?

	All areas specified by client including cavities, walls, roofs etc 

	Identify the Persons at Risk:
	Employees
	
	Contractors
	
	Public
	

	Name the substance involved in the process, the quantity and its manufacturer.
(A copy of a current safety data sheet for this substance should be attached)

	Quantities will vary dependant on the roof area & job specification.
Manufactured by ROCKWOOL.


	 Explain why a safer alternative cannot be used:

	The material and quantity has been specified by the client.	

	Classification (tick all that apply):

	Physical Hazards

	Unstable Explosive
	Flammable
	Oxidising
	Compressed Gas
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	

	Health Hazards
	Environmental

	Toxic
	Corrosive
	Irritant
	Resp. Sens/Health
	Environmental
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	

	Hazard Type:

	Gas
	Vapour
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other:

	
	
	
	
	
	
	
	

	Route of Exposure:

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (State)

	
	
	
	
	

	Explosive Limits and Workplace Exposure Limits (WELs) 

	Long-term exposure level (8hrTWA):
	Short-term exposure level (15 mins):

	
	
Respirable Dust – 15min STEL 5mg/m3














	Detail Potential Health Risks:

	Skin contact:
There may be mild irritation at the site of contact.
Eye contact:
There may be irritation and redness.
Ingestion:
There may be irritation of the throat.
Inhalation:
There may be irritation of the throat with a feeling of tightness in the chest.

	Control & Recovery Measures Actioned: (for example extraction, ventilation, training, supervision).  Include special measures for vulnerable groups, such as disabled people and pregnant workers.  
Take account of those substances that are produced from activities undertaken by another employer’s employees.

	Ventilation:
	Accidental Release & Spillage Plan :

	No Specific measures. 
	Transfer to a closable, labelled salvage container for
disposal by an appropriate method.

	Special Transport:
	Signage, provision of information and instruction :

	N/A
	Breifing this assessment 

	Fire Precautions/Extinguisher Type:
	Environmental Considerations :

	Suitable extinguishing media for the surrounding fire
should be used.
	Do not discharge into drains or rivers.

	Storage Required:
	Disposal Issues:

	Store in a cool, well ventilated area. Keep container tightly
closed.
	Disposal operations: Transfer to a suitable container and arrange for collection
by specialised disposal company.
Disposal of packaging: Dispose of as normal industrial waste.

	Is health surveillance or monitoring required for foreseeable exposure potential?

	Routine health screening
	No
	Personal air monitoring
	No
	Background air monitoring
	No

	Personal Protective Equipment (state type and standard)

	Item
	Tick
	Requirement
	Item
	Tick
	Requirement
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	Wear goggles to EN 166 is advised.
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	Use gloves conforming with EN 388 
	[image: ]
	
	Cover exposed skin.
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	Other
	
	

	First Aid Measures

	Skin contact:
Wash immediately with plenty of soap and water.
Eye contact:
Bathe the eye with running water for 15 minutes.
Ingestion:
Wash out mouth with water.
Inhalation:
Consult a doctor.

	Disposal Instructions for substance and empty containers:

	Hazardous Waste
	
	General Waste
	

	Return to Depot
	
	Return to Supplier
	

	Other/Notes:

	

	Is exposure adequately controlled?
	Yes
	
	No
	

	Risk Rating Following Above Controls:
	High
	
	Med
	
	Low
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