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Description automatically generated]SF16A COSHH Assessment Form
	COSHH Assessment for:
	No Nonsense Line Marking Paint
	Ref:
	506

	Assessor:
	Dom Reddall
	Date:
	June 2023
	Next Review:
	June 2026

	Describe the activity or work process:

	Spray paint used for line marking

	What is the location of the activity or work process?

	Used on site.

	Identify the Persons at Risk:
	Employees
	
	Contractors
	
	Public
	

	Name the substance involved in the process, the quantity and its manufacturer.
(A copy of a current safety data sheet for this substance should be attached)

	No Nonsense Line Marking Paint
Quantity to be used is as per job specification.
The minimum amount possible will be used.

	 Explain why a safer alternative cannot be used:

	N/A

	Classification (tick all that apply):

	Physical Hazards

	Unstable Explosive
	Flammable
	Oxidising
	Compressed Gas
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	

	Health Hazards
	Environmental

	Toxic
	Corrosive
	Irritant
	Resp. Sens/Health
	Environmental
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	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	
	Applicable:
	

	Hazard Type:

	Gas
	Vapour
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other:

	
	
	
	
	
	
	
	

	Route of Exposure:

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (State)

	
	
	
	
	

	Explosive Limits and Workplace Exposure Limits (WELs) 

	Long-term exposure level (8hrTWA):
	Short-term exposure level (15 mins):

	PETROLEUM GASES, LIQUEFIED; PETROLEUM GAS -
WEL 1000 ppm 1750 mg/m³
Acetone - WEL 500 ppm 1210 mg/m³
Butyl Acetate – 
150 ppm 724 mg/m³
SOLVENT NAPHTHA, LIGHT AROMATIC –
WEL 25 ppm 50 mg/m3(Sk)
Cumene - WEL 25 ppm(Sk) 125 mg/m3(Sk)
MESITYLENE - WEL 25 ppm 125 mg/m³
	PETROLEUM GASES, LIQUEFIED; PETROLEUM GAS <0.1% 1,3 BUTADIENE - WEL 1250 ppm 2180 mg/m³
ACETONE - WEL 1500 ppm 3620 mg/m3
Butyl Acetate - WEL 200 ppm 966 mg/m³
Cumene - WEL 50 ppm(Sk) 250 mg/m3(Sk)


	Detail Potential Health Risks:

	H222 Extremely flammable aerosol.
H229 Pressurised container: may burst if heated.
H319 Causes serious eye irritation.
H336 May cause drowsiness or dizziness.
H412 Harmful to aquatic life with long lasting effects.

	Control & Recovery Measures Actioned: (for example extraction, ventilation, training, supervision).  Include special measures for vulnerable groups, such as disabled people and pregnant workers.  
Take account of those substances that are produced from activities undertaken by another employer’s employees.

	Ventilation:
	Accidental Release & Spillage Plan :

	Provide adequate ventilation.
	Eliminate all sources of ignition. No smoking, sparks, flames, or other sources of ignition near
spillage. Provide adequate ventilation. Wear suitable protective equipment, including gloves,
goggles/face shield, respirator, boots, clothing, or apron, as appropriate. Provide adequate ventilation. Contain spillage with sand, earth, or other suitable non-combustible material. Avoid
the spillage or runoff entering drains, sewers, or watercourses. Absorb in vermiculite, dry sand
or earth and place into containers.

	Special Transport:
	Signage, provision of information and instruction :

	This product is packed in accordance with the Limited quantity Provisions of CDGCPL2, ADR
and IMDG.
	Brief this assessment and attached data sheet.

	Fire Precautions/Extinguisher Type:
	Environmental Considerations :

	Fire Precautions/ 
Extinguisher Type: Extinguish with alcohol-resistant foam, carbon dioxide or dry powder.
	Do not allow into waterways, drains or soil. Harmful to aquatic organisms.

	Storage Required:
	Disposal Issues:

	
	

	Store at moderate temperatures in dry, well ventilated area. Keep away from heat, sparks and
open flame. Pressurised container: Must not be exposed to temperatures above 50°C
	Dispose of as hazardous waste.

	Is health surveillance or monitoring required for foreseeable exposure potential?

	Routine health screening
	No
	Personal air monitoring
	No
	Background air monitoring
	No

	Personal Protective Equipment (state type and standard)

	Item
	Tick
	Requirement
	Item
	Tick
	Requirement
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	Use face fitted type P3 mask if ventilation is inadequate.
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	Safety Glasses (EN 166 ) to protect from splashes.
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	Wear impervious nitrile gloves complying with EN374-2.
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	Long sleeve clothing to prevent skin contact.
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	Other
	
	

	First Aid Measures

	General information - Move affected person to fresh air at once. Get medical attention if any discomfort continues.
Never give anything by mouth to an unconscious person.

Inhalation - Move affected person to fresh air at once. If breathing stops, provide artificial respiration. Keep affected person warm and at rest. Get medical attention immediately.

Ingestion - Rinse mouth thoroughly with water. Do not induce vomiting. Get medical attention.

Skin contact - Wash skin thoroughly with soap and water. Get medical attention if any discomfort continues.
Eye contact Rinse immediately with plenty of water. Continue to rinse for at least 15 minutes. Remove any contact lenses and open eyelids wide apart. Get medical attention immediately. Continue to rinse.

	Disposal Instructions for substance and empty containers:

	Hazardous Waste
	
	General Waste
	

	Return to Depot
	
	Return to Supplier
	

	Other/Notes:

	

	Is exposure adequately controlled?
	Yes
	
	No
	

	Risk Rating Following Above Controls:
	High
	
	Med
	
	Low
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