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	Contractor 
	Name: 
 
NFS Flooring UK 
Ltd 
	Address: 
83 Ducie Street 
Manchester 
M1 2JQ 
	Tel: 0161 945 8475 

	
	
	
	E-mail: 
info@naturalflooringsolutions.co.uk 

	Project Name 
	Fourways Manchester 

	Description of the Task/Activity 
	Timber flooring repair light sand & oil 

	Site 
Address/Location: 
	Fourways 
57 Hilton Street 
Manchester 
M1 2EJ 
	Start 
Date/Time: 
	16/07/2024 @ 18:00 

	
	
	Finish 
Date/Time 
	01/08/2024 @ 06:00 

	 
 
 
 
 
Personnel 
Involved 
	Name 
	Role/Trade 

	
	Michael Richardson 
	Site Supervisor 

	
	Said Benbrahim 
	Floor sander 

	
	Ayuub Benbrahim 
	Floor sander 

	
	Rachid Benjabour 
	Floor sander 

	
	Richard Meddani 
	Site Supervisor 

	
	  Kieran Coackley 
	  Floor sander 

	
	 
	 

	
	 
	 

	
	 
	 

	
	 
	 

	 
Site Supervisor: 
	Richard Meddani 
	 
Tel: 
	07796 652432 

	 
Safety Officer 
	Richard Meddani 
	 
Tel: 
	 

	 
Key Plant & Tools 
	Kunzle and Tazin Taurus belt sander x 5 Kunzle and Tazin Silverback edge sander x 3 Kunzle and Tazin Golia x 1 

	 
Key Materials 
	 
Osmo Polyx-Oil Raw & Osmo Polyx clear 

	 
Other Essential Equipment: 
	Festool RDA sanders x 3 / Festool dust extractors x3 / festool Kapex chop saw / Festool plunge saw & table saw / Fein multi tool x 5 / Dewalt cordless drills  

	 
Specific Identified 
Residual Hazards: (or refer to the task specific risk assessment(s)) 
	Bags of dust may combust Inhalation of dust. 
Noise emissions from sanding machines 
Machinery cable 
Wet lacquered floors 
Blocking emergency exit/doorways/hallways 
Lifting and transporting 
Dust Emissions 
Hand-arm vibration 
Fire 
Electrical 
Eye injury 


 
 
	 
 
 
 
 
	Conservation statement 

Sanding will take place as per approved sample as advised by the conservation team. We aim to remove the top layer of existing lacquer ONLY and maintain the grain to the original floorboards. We will aim to remove no more that 1mm throughout, taking care to do the sanding works gradually and methodically in an attempt to avoid over sanding.

Please refer to method statement for further information and grit ratings. 

Method Statement

· We will arrive at site and park in a designated safe area. 
 
· We will undergo a full site induction by the Principal Contractor. 
 
· Our Site Supervisor will walk around the site and carry out a Point of Work Risk Assessment to identify any specific hazards and controls not originally identified. The Site Supervisor is responsible for any amendments to the RAMS during the project. 
 
· Our Site Supervisor will deliver the contents of the RAMS to the workforce using a toolbox talk method. 
 

· All tools and equipment will be visually inspected prior to use and defects reported to the Site Supervisor immediately. 
 
 
· Doors and windows will be opened to ensure adequate ventilation and through flow of air and operatives will wear P3 respirators. All nonessential personnel will be removed from the area. 
 
· We will assess the damaged boards and replace using reclaimed pine floor boards to match existing. 
 
· Replacement floor boards will be fixed down using a face nail method to match existing. 
 
· All replacement boards with be cut to start and finish on existing joists. 
 
· The sanding process will commence using a Kunzle and Tasin belt sander and a Kunzle and Tasin edge sander. 
 
· This will be rotated amongst the workforce to minimize exposure to hand arm vibration.  
 
· All none essential personnel will be removed from the working area. 
 
· Signs will be posted on doors warning of the noise hazard present. 


· Running through the following abrasives: 

· 40 grit
· 60 grit 
· 80 grit



	 
	

	 
	60 grit 

	Sequence of Operations: (include sketches if required) 
	80 grit 
 
All edges will be finished with a 40 grit then a 80-grit using a Festool Rotex sander 

	 
 
 
	All sanding equipment has dust extraction allowing us to sand at 95% dust free 
Once sanding is complete, we will use a wet mop or ‘M’ Class vacuum to clear any dust deposits, we will NOT use a dry brush. 
we will apply 2 coats of Osmo Raw Oil/\Osmo clear hardwax oil using an Osmo brush applicator with a light buff between each coat. 
 
Doors and windows will be opened to ensure adequate ventilation and through flow of air and operatives will wear P3 respirators. All none essential personnel will be removed from the area. 
 
All dust bags will be removed from site at the end of each working day and disposed of properly. 

	 
 
	Single use overalls to be used and disposed of at the end of shift to prevent dust to be taken home. 
All wet areas will have signs and barrier tape making clear that no foot traffic is allow for the duration whilst products are drying 



	 
Temporary 
Supports and Props needed to facilitate the works: 
	None 

	 
Method of Access and Egress to the work area: 
	Access to site is via the main entrance  
 
Sign in on arrival and sign out on departure. 
 
All equipment and materials will be off loaded and loaded at the main entrance. 

	 
Fall Protection Measures: 
(Where work at height cannot be eliminated – consider both Personnel & 
Materials) 
	N/A 

	Storage 
Arrangements: 
	 
None 

	SWL’s: 
	N/A 




[image: ]
 
  
 
 
 
 
 
All work will be undertaken by qualified competent persons with experience of the type of work described above, and in all cases in full accordance with safety procedures specified in the company’s Health and Safety Policy. 
 
	 
Prepared by: 


 
Kathryn Foran 

	 
 
Position: 
 
 
Reviewed by: 
 
 
Position: 


 
Secretary 
Date: 11/07/2024 
 
 
Richard Meddani 
 
Manager 
Date: 11/07/2024 
 
 
	Items Attached: 
	Yes 
	No 

	Sketches 
	
	  

	Program of Work 
	
	  

	Risk Assessments 
	
	  
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Required Personnel
Protective
Equipment:

Safety Boots

Safety Gloves Hearing Eye Protection Respiratory
Protection (when Protection
required) P3 face fit

tested

Other:

Hi-Viz vest

Disposable
Overalls

Kneepads.

Emergency Procedures:

First Aid
Facilities:

<4
D

Name of On-Site First
Aider:

Richard Meddani

Van/Storage area on site
First Aid Box Location:

MRI

Oxford Road
Manchester
M13 9WL

Location of Nearest

Hospital:
Tel: 0161 276 1234

Welfare Requirements

Facilities provided on site

of CDM 2015.
Services to be supplied by
Others N/A

None

Other information &
Comments
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