Construction Management Plan  Planning Ref 129138 /FO/21
Land off Dukefield Street Manchester M22 4WQ

Work will be carried out by Fitzgerald Builders ,1 Chapel Road, Manchester M22 4JN
Tel 0161 998 7673 
Emergency number 07961301993
Local residents will be contacted in writing confirming the start date working hours and emergency contact.
Dust Suppression measures:
All plant and equipment shall be maintained in accordance with manufacturer’s recommendations to ensure emissions to atmosphere are minimised.
 ii) Engines of plant, machinery, and lorries shall be turned off at all times when not in use.
 iii) Delivery activities, plant, stockpiled materials and/or any other activities liable to significant dust generation shall be located as far away as possible from the development site boundaries and neighbouring properties.
iv) Stored materials liable to dust generation shall be dampened down, covered with tarpaulin, or otherwise contained as far as reasonably possible. 
v) Drop heights from conveyors, loading shovels, hoppers, and other loading or handling equipment shall be minimised and fine water sprays should be used on equipment where necessary. 
vi) Skips, chutes, and conveyors shall be covered and if necessary enclosed to ensure that dust does not escape. 
vii) All vehicles carrying dusty materials shall be securely covered. 
viii) Water suppression shall be used in dry conditions to reduce dust emissions (e.g. mobile bowsers or fixed sprayers as appropriate). 
ix) Areas where there is regular vehicular movement should have a consolidated surface which shall be kept in good repair.
Waste Materials
There shall be no burning of waste materials on site at any time
Waste materials will be kept to a minimum and placed in secure skips for recycling or disposal at a licensed waste management site
Parking and routing of construction vehicles
Deliveries to the site will be organised outside rush hour to minimise disruption on the main road 
The work will be carried out by a small in house team without the need for sub contractors thereby reducing the number of vehicles visiting the site .
Sheeting over of construction vehicles
All vehicles carrying dusty materials shall be adequately covered.
Washing of contractor wheels and access roads
There will be facilities on site to wash down  vehicles leave the site to avoid any mud being deposited on the access road.



