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HDPE Chamber - 610mm diameter x 1000mm tall

Pedestrian Duty Cover & Frame - 450mm diameter

10mm Rubber Inlet Seal

7 Check / Non-Return Valve

63mm MDPE Tank Connector

2" PVC Pipework
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Foul/ Sewage Pump with Float

‘Additional Information:

Position of inlet seal (C) is shown for iiustration purposes only
actual position of nlet seal will be cut by customer on site
relevant o drainage position requirements.

Solids Handling capacity of this foul / sewage pump is S0mm.
All standard pumps supplied are single phase and require &
240V supply unless a different pump has been requested. An

electrician is required to safely connect this pump to the mains.
If you require further advice, please contact us
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