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Attenuation Tanks – Versa void Modula Geo-Void 

Maintenance 
ESS Geo-void modular tank system provides total all round access with clear access point and channels in all directions.
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Pumping chamber – Kingspan 
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Foul/rainwater & Grey water drainage including manholes

All drainage for the scheme is internal either at ground floor or at basement level. No external drainage is connected to the waste. The scheme is design to utilise a combined outlet manhole which is existing with all drainage internal of this being split. To maintain this drainage, it requires a 12 monthly flush with clean water and any blockages can get cleared from internal manholes. The basement foul drainage is connected to the pumping station above to prior to entering the combined manhole (follow maintenance strategy above for this). 
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6 General Maintenance

The best way to achieve this is to arrange a contract with an approved Service provider. Please contact us on the
phone number given for service contact details.

There will always be situations when a little self help may be sufficient to avoid call out and we describe here
some basic checks which may prove useful: Before opening the unit, please see Health and Safety Notes.

We recommend the unit is checked every 6 months to ensure there are no blockages or obstructions in the inlet
and out let pipes, also check that there is not excessive sludge build up in the bottom of the tank.

If in any doubt whatsoever please contact your service provider.
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