1. Confirm size of site.

0.19 hectares

2. Is the boundary wall being demolished.

No the boundary wall will be retained.  

3. Can we have a plan showing the proposed boundary treatment.

As per question 2, the boundary treatment will be retained as existing. 

4. How will rubble and waste be removed from site?

Waste will be disposed of on site by third parry haulage company appointed by MJ Finnigan Ltd. Wagons to be covered to minimise dust. Road sweepers used on completion as required. 

5. Adequate segregation of pedestrians and vehicle traffic will be maintained at all times. Reversing of vehicles and plant will be minimised at all times. This will be highlighted on a site plan and will form part of the site induction for all operatives.

MJ Finnigan confirm this is carried out as part of our site induction process. 

6. Can you confirm the Site working hours. 

07.30 – 16.30 Monday – Friday.  8.30am – 2pm Saturday.   We understand these are standard MCC working hours.  The programme for demolition will take place over a 1 week period. 

7. Can you confirm that Hazardous waste stored under COSHH regulations, disposed of separately and that the following will take place:
· Daily cleaning of areas.
· All carriers of waste will hold valid transfer licences and provide
certification to the principal contractor

No hazardous waste on site 

8. Can you confirm the following :To reduce the volume of waste sent to landfill waste from Site will be segregated at the main collection point for debris produced in the following categories: 
 CAT A – Hazardous waste (paints, thinners, mastics etc.); 
 CAT B – Metal; 
 CAT C – Timber; 
 CAT D – Plasterboard; and 
 CAT E – General Waste 

Waste transfer notes will be issued for all waste materials removed from the site.   MJ Finnigan confirm the above and all waste transfer notes will be issued as part of the handover. 

9. The submitted Method Statement refers to Pyes Yard on Hoyle Street – can this be updated to reflect the correct site. 

Please see attached revised RAMS

10. Can you confirm that any rubble (that cannot be recycled) will be disposed off site in a licenced facility.

All material will be recycled in line with MJF sustainability policy – with the exception of asbestos which will be taken to landfill and waste notes provided 

11. Can we have  a copy of the Asbestos Survey.

Deloitte has provided a copy of this to the LPA. 

12. Can you confirm that strict noise monitoring measures will be introduced to ensure that plant and site activity noise levels do not exceed reasonable increase in dB levels when assessed against site specific background noise.

Noise will be controlled / minimised as follows:-
· By ensuring that the equipment and plant is well maintained and operating within their design noise parameters, in accordance with Manufacturer’s instructions. We shall also follow BS5228 - Code of Practice Noise Control on Construction and Demolition Sites.
· The Site Supervisor will ensure that supplies of ear defenders or other hearing protection is made available where it is not possible to reduce the noise level to a safe limit.  
· The Site Supervisor will ensure that all noise control items fitted to plant and equipment are kept in good order and that any defects noted are reported to the Plant Manager or Hire Company immediately.

13. Can you confirm that there will be no material crushed on site and no burning of rubbish on site.  

There will be no material crushed nor burnt on site.  Details of waste categorisation and transfer are set out in the RAMs Method Statement which has been updated and provided alongside this note.
