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	SYSTEM TYPE
	Description 

Refer to FK Façade Performance specification for details
	General area of the building. 

Refer to Façade Type Elevations (21000) series) drawings for exact locations of each façade type. 
	External finish and colour
(all finishes and colours subject to planning condition approval and discharge)
	Internal finish and colour
	Sign off Date

	EWS-01
	Vertical Curtain Walling SSG (unitised) 

SSG vision glazed curtain walling. External capless joints. Alternating bronze anodised articulated vertical fins and spandrel panels. Spandrel Panel. 
	‘Honeycomb’ façade to 02-05 office floors


	Spandrel - opaque glass internal frit colour: RAL 7011

(dark grey / blue)
Architectural Fin: 

Aluminium finish: anodised

Colour: Anodised Analok 543

(bronze)

Door frames / trims

Aluminium finish: anodised

Colour: Anodised Analok 543

(bronze)

Uppermost / perimeter roof cap 

Aluminium finish: PPC
Colour: RAL 7011

(dark grey / blue)


	Finish: PPC

Colour: RAL 7011

(dark grey / blue)
(60/40 - Matt/Gloss)
Terrace Mullions 

Finish: PPC

Colour: RAL 7011

(dark grey / blue)
(60/40 - Matt/Gloss)

	28/01/25

	EWS-02
	Vertical Curtain Walling (Stick)

Capped vision glazed curtain walling. Based stacked systems are proposed. Spandrel Panel. 
	Ground and level 1
	Capping & Door frames/trims Aluminium finish: anodised

Colour: Anodised Analok 543

(bronze)

Spandrel – opaque glass internal frit colour: RAL 7011

(dark grey / blue)

	Finish: PPC

Colour: RAL 7011

(dark grey / blue)
(60/40 - Matt/Gloss)

	09/05/25

	EWS-02a
	Vertical Curtain Walling (Stick)

Silicon glazed curtain walling. Based stacked systems are proposed. Spandrel Panel. 
	Ground and level 1
	Silicone bonded finish externally in lieu of capping.

Door frames/trims
Aluminium finish: anodised

Colour: Anodised Analok 543

(bronze)

Spandrel – opaque glass internal frit colour: RAL 7011

(dark grey / blue)

	Finish: PPC

Colour: RAL 7011

(dark grey / blue)
(60/40 - Matt/Gloss)

	09/05/25

	EWS-02b
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	Vertical Curtain Walling with Shadowbox and or other feature highlight.

Etail to be confirmed in later stages with input from client/occupier.
	Level 1
	TBC 
	TBC 
	09/05/25

	EWS-03
	Vertical Curtain Walling SSG (unitised) 

SSG vision glazed curtain walling. External capless joints. 
	Level 06 office. 


	Spandrel - opaque glass internal frit colour: RAL 7011

(dark grey / blue)

Door frames / trims

Aluminium finish: anodised

Colour: Anodised Analok 543

(bronze)

Uppermost / perimeter roof cap 

Aluminium finish: PPC
Colour: RAL 7011

(dark grey / blue)


	Finish: PPC

Colour: RAL 7011

(dark grey / blue)
(60/40 - Matt/Gloss)
Terrace Mullions 

Finish: PPC

Colour: RAL 7011

(dark grey / blue)
(60/40 - Matt/Gloss)

	28/01/25

	EWS-04
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	Louvre 
	Loading bay
	Aluminium finish: PPC Colour: Y2206F Steel Bronze 1 reference is within the Interpon D2525 Anodic Collection. 
	N/A
	09/05/25

	EWS-05
	Blockwork wall
	Gridline 10 – Link facade
	N/A
	N/A
	09/05/25

	EWS-06

	Acoustic louvre
	To plant areas level 7
	Aluminium finish: PPC Colour: Y2206F Steel Bronze 1 reference is within the Interpon D2525 Anodic Collection.


	
	

	EWS-07

	Unitised Curtain Wall Panel/Cassette with                              render finish
	201 Deansgate Level 02-06
	Render finish to best match the GRC – Pura Facades, Cotton Ferro Light.
Dryvit 101 Stone Mist Castle Grey

Supplier to propose dryvit samples. 

	N/A
	09/05/25

	EWS-07a
	Curtain Wall Louvres with stone finish
	201 Deansgate Level 02-06
	TBC
	N/A
	09/05/25

	EWS-08
	Vertical Curtain Walling SSG (unitised) 

SSG vision glazed curtain walling. External capless joints. Alternating bronze anodised articulated vertical fins and spandrel panels. Spandrel Panel. 
	‘Honeycomb’ façade to tower floors.

Different bay ratios and floor to floors to podium.

	Spandrel - opaque glass internal frit colour: RAL 7011

(dark grey / blue)
Architectural Fin: 

Aluminium finish: anodised

Colour: Anodised Analok 543

(bronze)

Uppermost / perimeter roof cap 

Aluminium finish: PPC
Colour: RAL 7011

(dark grey / blue)

	Finish: PPC

Colour: RAL 7011

(dark grey / blue)
(60/40 - Matt/Gloss)

	28/01/25

	EWS-08a
	Horizontal Perforated Fin as part of Vertical Curtain Walling SSG (unitised) 


	‘Honeycomb’ façade to tower floors.

9mm diameter perforations

	Perforated Architectural Fin: 

Aluminium finish: anodised

Colour: Anodised Analok 543

(bronze)

	Finish: PPC

Colour: RAL 7011

(dark grey / blue)
(60/40 - Matt/Gloss)

	16/01/26

	EWS-09
	Vertical Curtain Walling SSG (unitised) 

SSG vision glazed curtain walling. External capless joints. The design includes a ‘double transom’ at floor slab levels.
	Gable end tower floors


	Spandrel - opaque glass internal frit colour: RAL 7011

(dark grey / blue)

Door frames / trims

Aluminium finish: PPC
Colour: RAL 7011

(dark grey / blue)

Uppermost / perimeter roof cap 

Aluminium finish: PPC
Colour: TBC
	Finish: PPC

Colour: RAL 7011

(dark grey / blue)
(60/40 - Matt/Gloss)
Terrace Mullions 

Finish: PPC

Colour: RAL 7011

(dark grey / blue)
(60/40 - Matt/Gloss)

	28/01/25

	EWS-10



	Rainscreen
	Curtain Wall to ‘neck’
	Aluminium finish: PPC
Colour: RAL 7011

(dark grey / blue)


	N/A
	09/05/25

	EWS-11
	Vertical Curtain Walling SSG (unitised) 

SSG vision glazed curtain walling. External capless joints. The design includes a ‘double transom’ at floor slab levels.
	Curtain Wall to penthouse
	Spandrel - opaque glass internal frit colour: RAL 7011

(dark grey / blue)

Door frames / trims

Aluminium finish: anodised

Colour: Anodised Analok 543

(bronze)

Uppermost / perimeter roof cap 

Aluminium finish: anodised

Colour: TBC
	Finish: PPC

Colour: RAL 7011

(dark grey / blue)
(60/40 - Matt/Gloss)
Terrace Mullions 

Finish: PPC

Colour: RAL 7011

(dark grey / blue)
(60/40 - Matt/Gloss)

	28/01/25

	EWS-12
	Rainscreen Aluminium with bronze finish
	Bootle street and 201 Deansgate level, 00-02
	Aluminium finish: PPC Colour: Y2206F Steel Bronze 1 reference is within the Interpon D2525 Anodic Collection. 

	N/A
	09/05/25

	ESW-12a
	Rainscreen Aluminium Louvres with bronze finish
	201 Deansgate level 00
	Aluminium finish: PPC Colour: Y2206F Steel Bronze 1 reference is within the Interpon D2525 Anodic Collection. 
	N/A
	09/05/25

	EWS13
	Withdrawn


	N/A
	N/A
	N/A
	N/A

	EWS 14

	Column and header wrapping to base of Podium

GRC panel concealed  fixings on helping hand brackets back to structural column.
	Found at level 00-01 at columns and header fascia to surround of building. 
	Pura Facades – Cotton Ferro Light.
	
	09/05/25


No.2 St. Michael’s 


Stage 4 





Façade finishes schedule
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P06: Inclusion of Perforated Horizontal Fins EWS-08a
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