Extension to form 8 new 2-bedroom flats to the rear of: 
83 – 95 Wendover Road, M23 9EG
External Finishes Specification
1. External Walls
1.1 Brickwork (Below DPC and to Floor Level)
· Damp Proof Course Zone:
· Two courses of red engineering bricks to be installed up to DPC level.
· Bricks to be Class A or B engineering grade, providing high durability and low water absorption.
· Brickwork to Floor Level:
· Above the engineering brick courses, walls to be constructed in Scotch Common bricks up to finished floor level.
· Brickwork to match existing property tones where applicable.
1.2 Rendered Elevations
· All elevations above floor level to receive a white K‑Rend finish.
· Render system to be through‑coloured, providing a durable, low‑maintenance surface.
· Finish to be smooth or scraped texture (as agreed with client/LA), consistent across all elevations.
2. Windows and Doors
· All new windows and external doors to be white uPVC.
· Frames to be energy‑efficient, double‑glazed units meeting current Building Regulations, installed as per drawing 0824/01/54 (Condition 4)
3. Roofline Components
3.1 Fascias and Soffits
· New fascias and soffits to be white uPVC.
3.2 Rainwater Goods
· All gutters, downpipes, and associated fittings to be black uPVC.
· System to be half‑round or square profile, installed to manufacturer’s recommendations.



4. General Notes
· All materials to be installed in accordance with manufacturer specifications and relevant British Standards.
· Any variations to the above specification must be agreed with the client and, where required, the Local Planning Authority.
· Samples of bricks, render, and uPVC components may be requested for approval prior to installation.

