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MAINTENANCE INSTRUCTIONS & CLEANING FOR GALVANISED STEEL

Product  :-  Steel handrails / steel / gates /rails/staircase
Material :- Mild Steel
Coating  :-  Galvanised Finish (Hot Dip) & powdercoated

               All Material is galvanised BSEN1461. 

1) To maintain the quality of the items, avoid any scratching of the surfaces, this will ensure that no corrosion occurs to any of the steel.


2) To clean the steel  use of water and simple soap or disinfectant without scrubbing or scratching of the surfaces will maintain the coating.

3) Should any scratches or breaks in the coating occur, preventing corrosion can be ensured by use of either a zinc primer or galvanising touch up paint or recoating with powder to match where required.
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