24.08.26 – Mock up for approval
Protection to the concrete column – 10mm high density foam pad placed behind each steel uni-strut channel/ section.
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