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The Northern Tennis Summary

The Northern lighting design has been completed to the requirements for environmental zone 4, this is the expected requirement due to an urban environment with high level of street lighting, building façade lighting and sports lighting within the local environment to the Northern tennis Club.

The E4 lighting recommendation for window lux levels within this zone is 25 lux max. 

P28 of the lighting report details the highest reading of a window in the environment at 22.8 lux average 24.9 lux max. many of the other windows measured are lower than 15 lux.

P3 details an image of the number of windows measured, with all local windows in Elm road and Blackburn Gardens included with the max results shown in the PDF print. All window lighting results are available, the highest results were shown only to reduce the report size.

There are no physical obstructions ( even boundary walls ) entered into the design to give a worst case rendered scenario.
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