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Cornthwaite Tree Care, Unit 10 Crosse Hall Works, Crosse Hall Street, Chorley PR6 0QQ

___________________________________________________________________________________________________________________________________________

10.1
Emergency Contingencies 
	Ref
	Hazard
	Risks
	Persons involved
	Initial Risk
	Industry best practice/guidance
	Further information
(for those at risk)
	Control measures
	Residual risk

	10.1.1
	Staff or other personnel on site suffer injury, including infection with communicable disease, e.g. HIV, Hepatitis A or B, and TB

See also 10.2.2 Disease and infection
	Fatality, ill health, worsening of condition, complications.   Viral infection, psychological trauma
	Work team/ client/general public
	Intolerable 
4-High


	Guidance Notes: HSE BBV’s In work place (INDG342).

Health monitoring and surveillance
	INDG 342 Blood Born Virus Guidance
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	Appropriate First Aid Kit on site.   
Staff trained and certificated in First Aid.   
Staff know site location and means of contacting emergency services. Only remove hypodermic syringes from site with approval and using appropriate equipment before other work commences, if  there is a large amount of syringes call for specialist assistance to clear the site
	Tolerable
   1-Low

	10.1.2
	Fire/explosion
	Burns/blast injuries
	Work team/ client/general public
	Intolerable 

4-High


	FISA Safety Guide 802-803 HSE HSG47 “Avoiding danger from underground services” INDG 370 Controlling fire at work


	HSG47 Avoiding danger from underground services
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INDG 370 Controlling fire at work
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	Appropriate First Aid Kit on site.   

Staff trained and certificated in First Aid as above and fire extinguishers fitted in works vehicles and at work locations sited in the spill kits at refuelling points, staff trained in their use
	Tolerable

Low-1

	10.1.3
	Contact with energised power lines

See also 10.2.3 Power lines – over and underground
	Serious injury/ fatality.  Third party electrocution.
	Work team/ client/general public
	Intolerable 

4-High


	Arb Association Tec-guide 1 Tree Climbing & Aerial Rescue

 FISA Safety Guide 802, 804
HSE HSG47 “Avoiding danger from underground services”
GS6 Avoiding danger overhead power lines
Electricity at work SW P
	HSG47 Avoiding danger from underground services
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GS6 Avoiding danger overhead power lines
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Electricity at work SWP
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	Staff trained.   Emergency procedures known.   Accurate assessment of situation.   Means of contacting Regional Electricity and other utility Company are known to all staff, obtain copies of all utility services paying attention to under-ground service maps from relevant companies prior to commencing work
Escape route and Rescue plan approved and briefed Appropriate First Aid Kit on site.   

Staff trained and certificated in First Aid.
	Tolerable

Low-1

	10.1.4
	Emergency call-out work including

Night-time work. 
Poor weather conditions.
	Cut/crush/ impact injury due to poor visibility/ unstable trees or structures/ other people/ vehicles on site.
	Work team/ client/general-public
	Intolerable 

4-High


	Arb Association Tec-guide 1 Tree Climbing & Aerial Rescue

Arb Association Tec-guide 2 use of Tools in the Tree

FISA Safety Guide 301, 302, 304, 306, 307, 310, 505, 801, 802, 804: HSE 
INDG317 Chainsaws at work
	         Chainsaws at work    
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	All operators trained and certificated.  Co-ordination with emergency service     (if deemed necessary) local authorities, utility company etc.   Portable lighting on site.   Unauthorised personnel excluded from work area: signs, barriers, etc. PPE.
	Tolerable

Low-1
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