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SIS Pitches End of Life Synthetic Turf Statement.
Any existing synthetic carpet will be fully recycled. The recycling is carried out at the only bespoke recycling plant in the UK.  100% of the synthetic surface is recycled, and the process has been continually refined to ensure minimal to no wastage, converting the entire surface into useable and high quality output product whether that be the rubber, the sand or the synthetic fibres that can be used in a large number of recycled plastic products.
The rubber granules will be separated from the pitch infill system, with the granules cleaned and graded as 0.8–2.5mm styrene-butadiene rubber based on precise particle sizing. The particles are then sampled and tested to ensure they meet current REACH compliance and SAPCA infill protocols before being sold back into the market as recycled material for new pitches at a lower price than virgin material
Once the sand has been isolated from the carpet system, it will be thoroughly cleaned, dried and graded to provide 'new' 0.2–0.7mm sand, which will be sold to be reused in new synthetic turf installations
After the rubber and sand have been removed from the carpet, the artificial turf rolls are then shredded, cleaned and processed. Sportex then use specialist plastic agglomeration technology to produce sustainable recycled plastic kickboard, which we will reuse for infill mitigation on future projects, thereby creating closed loop recycling, reducing waste sent to landfill.
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