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20/20 Antique Slate

Sandtoft

The 20/20 roof tile is a modern take on the traditional plain tile, using a modern interlock to provide
greater flexibility and performance. Pressed from natural alluvial Humber clay, this premium mater
delivers improved longevity and natural beauty. The clay's irregularity adds charm and texture to ai

Minimum Roof Pitch:

15° at a minimum of 100mm headlap
22.5° at a minimum of 75mm headlap
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Covering Capacity:
20.9 tiles per m2 at 75mm headlap

23.2 tiles per m2 at 100mm headlap

Technical Data

Maximum Weight Per Sqm

Quantity Per Pallet

Additional Information

Length x Width 330x 226 mm
Cover Width 191 mm
Hanging Length 300 mm
Profile Depth 16 mm
Minimal Batten Gauge 210mm

Maximum Batten Gauge 255 mm





