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Addendum to Method Statement
Note: This document is to be read, understood and signed in conjunction with the main Method Statement and Risk Assessment; it contains only a description of internal works installing traditional lath and plaster
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Additional Equipment Required not covered in main RAMS:

None

Description of Activities:

Once all previous plasterboards damaged by multiple years of water ingress have been removed the existing joists and rafters will be covered using Larch lath 25mmx6mm , anchored to the structure using stainless steel nails.

The basecoat CLM28F is then applied on to lath, containing Belmix Flock Fibres which are specifically engineered high-performance multifilament polypropylene fibres to replace the historic use of animal hair in a lime mortar. These fibres are an effective alternative to animal hair, assisting with reducing the potential of cracking and shrinkage and improving a lime mortar’s impact resistance. The fibres are polypropylene based. The flocking process allows for a greater surface contact area for the mortar matrix. 
 
Following sufficient time, CLM 28 Float coat is applied, again sufficient timer is allowed to enable the natural product to air.

The CLM 66 Fine plaster then gives it the fine appearance.
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	By signing this form, you also confirm that there have been no changes to your health since your last assessment that could impact on your ability to undertake the works proposed above.







Helix Roofing Contractors Ltd, 9 Breck Road, Wallasey, Wirral, CH443BB
Email: info@helixroofing.com
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