Hayescroft 
ALL REASON IN CAPITALS AFTER SPEC.
Phase 5 Work
Tree ID	
604	Sycamore. Fell to ground level. LIMITED POTENTIAL POOR CONDITION
605	Sycamore. Fell to ground level. LIMITED POTENTIAL POOR CONDITION
687	Irish Yew. Reduce in spread over the garden by 1.5-2 metres. TO MINIMISE OVERHANG OVER GARDEN DUE TO PROXIMITY TO PROPERTY.
689	Sycamore. Reduce in spread over the garden by 1.5-2 metres. TO REDUCE OVERHANG OVER THE BOUNDARY
690	Oak. Fell to ground level.  POORLY SITED TREE IN POOR CONDITION
699	Irish Yew. Crown lift over the path to a height of 4 metres. TO CLEAR THE PATHWAY
742	Sycamore. Fell to a 6 metre monolith. LIMITED POTENTIAL POOR CONDITION 
774	Horse Chestnut. Remove the large limb over the pavement/road. TO REDUCE OVERHANG AND CLEAR THE ROAD
Total cost to undertake Phase 5 (Four Year)
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