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PROPOSED RESIDENTAIL DEVELOPMENT
Greenwood / Gladeside Road
Wythenshawe


Project Details
Client: 
Challenger Building Services Ltd
Postal address:
140 Lee Lane,
Horwich,
Bolton,
BL6 7AF


Application reference: 125993/FO/2020

Brief description of the works:

Redevelopment of the site to provide 40 no. one and two bedroom affordable apartments, together with associated parking, amenity space and site infrastructure.













 List of the Proposed Materials
Brickwork
Type –Heywood Red Multi
[image: 059d0228-3994-48e2-badb-04723c6a07e2.JPG]


Parapet Roof Coping
Type – wall coping

[image: Arrow

Description automatically generated]

Windows
Type –UPVC – Grey
[image: Image from awmglass.co.uk]

External Doors (Apartments – Courtyard)
Type –  Composite Door – Colour Grey to Match Windows.

[image: ]

	

French doors
Type – UPVc French Door – (Grey)
[image: Text

Description automatically generated]

Juliette Balconies – Colour Black

[image: Steel & Glass Juliet Balconies | BA Systems]


Rainwater Goods
Gutter detail within single ply roofing system
[image: A picture containing concrete

Description automatically generated]



Marley anti vandal RWP and hopper

[image: Diagram

Description automatically generated][image: Diagram, engineering drawing

Description automatically generated]






















Paving for Paths around Building
Marshalls Regent Concrete paving

[image: A picture containing outdoor, ground, sidewalk, building

Description automatically generated]



Paving 
Saxon Paving 450 x 450mm

[image: A picture containing floor, plant, garden, stone

Description automatically generated]
Block Paving
A&G Country Cobble – (Colour Cashel)

[image: ]















Access Road – Tarmac SMA

[image: A picture containing text, road, grass, outdoor

Description automatically generated]



Hooped top railings to front 

[image: A picture containing fence, building, gate

Description automatically generated]

Colour Black
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Downpipe 3m
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