Phase 4
Tree ID	
[bookmark: _Hlk148882595]561	Holly. Fell to ground level. LIMITED POTENTIAL/POOR CONDTION
572	Sycamore. Fell to ground level. LIMITED POTENTIAL/POOR CONDITION
579	Holly. Fell to 2 metres from ground level. LIMITED POTENTIAL/TO ALLOW LOWER TREE TO BE MAINTAINED
581	Holly. Fell to ground level. LIMITED POTENTIAL/POOR CONDITION
616	Sycamore. Fell to ground level. LIMITED POTENTIAL/POOR CONDITION
698	Holly. Remove diseased stem. TO REDUCE RISK OF FAILURE
564	Holly. Reduce the decayed branch in spread by 3 metres. TO REDUCE RISK OF FAILURE
567	Holly. Reduce in height by 3 metres. TO REDUCE OVERALL SIZE OF CANOPY
570	Holly. Reduce spread from the driveway by 3 metres TO REDUCE OVERALL SIZE OF CANOPY TOWARDS DRIVE
575	Holly. Reduce spread from the driveway by 2 metres. TO REDUCE OVERALL SIZE OF CANOPY TOWARDS DRIVE
591	Holly. Reduce in height by 2 metres. TO REDUCE OVERALL SIZE OF CANOPY 
600	Holly. Reduce in height by 3 metres. TO REDUCE OVERALL SIZE OF CANOPY
702	Irish Yew. Crown Lift the primary branching to a height of 4 metres. £47.00+VAT £50.00+VA
743	Beech. Remove deadwood. Dead branch size >50mm. Reduce spread over parking by 1.5- 2 metres. TO LIMIT THE RISK OF LIMBS FAILURES/LIMBS FALLING OVER CAR PARK
538	Large Sycamore that has now 50 % died back. Sectional dismantle to the height of the main fork. Cost £2000.00+VAT EXTENSIVE SOOTY BARK DISEASE ON THE TRUNK OF THE TREE HEAVY DIEBACK OF THE CROWN.
668	Sycamore extensive bleeding on the main stem. Fell to the height of the main fork. DIEBACK OF THE CROWN AND EXTENSIVE BLEEDING ON THE STEM INDICATING LIMITED LONG TERM POTENTIAL
Trees at the rear of 14. See separate quote below previously provided for these trees, this has been adjusted in line with my most recent inspection.
1. Yew 0687 - Reduce in height by 2 metres and clip back on the property side by 1.5 metres. TO REDUCE SIZE DUE TO PROXIMITY TO PROPERTY
2. Yew 0688 - Crown lift by 1 metre. TO LIFT THE LOWER CANOPY
4. Yew No Tag - Reduce in height by 1.5 metres and prune lateral branches all around by 1 metre TO CONTROL SIZE DUE TO PROXIMITY TO PROPERTY

