Evidence to verify application for Certificate of Lawful Development at 7 Bankfield Ave, Longsight, Manchester M13 0YQ 

This proposal is for the construction of a loft conversion complies with Permitted Development Guidance as set out in the Planning Portal Website under Class C Development –

The current house:
· Is not a building containing one or more flats, or a flat contained within such a building
· Has not already had additional storeys added to it under permitted development rights
· Was not changed to be used as a house (from a previous non-residential use) under permitted development rights.
· Was not built as a ‘New Dwellinghouse’ under permitted development rights.
· Is not on Article 2(3) designated land*
Limitations on the proposed development:
· Materials must be similar in appearance to the existing house
· Volume of enlargement (including any previous enlargement) must not exceed the original roof space by more than:
· 40 cubic metres for terraced houses; or
· 50 cubic metres otherwise
· Must not exceed the height of the existing roof.
· On the principal elevation of the house (where it fronts a highway), must not extend beyond the existing roof slope.
· Must not include:
· verandas, balconies* or raised platforms; or
· installation, alteration or replacement of any chimney, flue, or ‘soil and vent pipe’
· Side-facing windows must be obscure-glazed; and, if opening, to be 1.7 metres above the floor of the room in which they are installed.
· Construction must ensure that:
1. The eaves of the original roof are maintained (or reinstated)
2. Any enlargement is set back, so far as practicable, at least 20cm from the original eaves (see pages 35-36 of the Technical Guidance below for more details)
3. The roof enlargement does not overhang the outer face of the wall of the original house


There are currently many loft conversions within the context of the dwelling with similar extensions and dormers. This addition will enhance the quality of life for the applicant and their family. All the 






	
