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21st November 2022
Manchester City Council

Planning

PO Box 532

Manchester

M60 2LA.

Dear Team,

Site: SLUG AND LETTUCE, 64-66 DEANSGATE, MANCHESTER, M3 2E
DESIGN AND ACCESS STATEMENT
Use

Pub and Restaurant
Amount 

Not applicable.  Our application is for signage / advertisements on an existing building and we are proposing no other development to the site with this application.

Layout

Please refer to block plan drawing no. 596664-5 for clarification of sign positions.

Scale

Not applicable.  Our application relates only to the installation of signage / adverts on an existing building.  We are not proposing any new buildings as part of this application.

Landscaping

Not applicable.  Our application relates only to the installation of signage on an existing building.  No new landscaping is to take place, or any existing landscaping impacted upon as part of this application.

Appearance

Please refer to drawing nos: 596664-1,2,3,4 and block plan no: 596664-5.  Please also refer to visual Slug and Lettuce Deansgate Rev B.

1 X SET OF HALO ILLUMINATED FASCIA TEXT TO REPLACE EXISTING – Positioned behind the window.  Built up letters have 1.2mm descaled stainless steel face rims and returns which are finished a dark gold color.  Flat cut 1.5mm ali inset letters are finished a lighter Ardenbrite Green Gold and are bonded within the front rims.  The backs are rebated 10mm opal acrylic.  Screw fixed to replacement black steel shs rails fixed behind the glazing and hanging from the ceiling.  Fitted with low energy white LEDS for halo illumination.
2 X INTERNALLY ILLUMINATED PROJECTION SIGNS - To replace existing Folded and welded 2.5mm ali panels are finished satin white and are fixed over a steel inner frame.  Text is fret cut into the panel faces and fitted with push through 8mm opal 030 acrylic letters.  Flat cut 2mm ali letters are finished Ardenbrite Green Gold no 3 and are bonded to the front of the acrylic.  Panels fix around a steel inner frame and the fixing arms are covered by a folded and welded white aluminum shroud.  Fitted with low energy white LEDS for halo illumination.  
2 X INTERNALLY ILLUMINATED MENUS – 1.2mm descaled stainless steel door and back box are finished matte Ardenbrite Green Gold No. 3.  6mm toughened glass. 5mm opal polycarbonate panel with cool with LED illumination.  Continuous stainless steel hinge and two chrome locks.  Screw fixed to the wall.
Our design team has looked at all aspects of creating a signage scheme to suit the Grade II listed building. We have always been aware to produce a design concept that compliments the surrounding conservation area and is sympathetic to the listed building. We feel the simple design compliments the building.
Access

Not applicable. Our application relates to signage / adverts only.  There will be no change to the current access arrangements as part of this application.
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