COSHH ASSESSMENT

	Task
	Use of Saint Astier Natural Hydraulic Limes (NHL)3.5

	Area / Location 
	Fraser House
	ASSESSMENT No
	COSHH 

	Assessed By
	John Russell & Jordan Beasley
	Date
	12th July 2022

	Title
	Health and safety advisor
	Review date
	As required

	Signal Word
	Danger

	The Substance – Hazard Identification

Please denote the properties of the substances used in the task 
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Corrosive (causes severe skin burns and eye damage), serious eye damage
Respiratory sensitiser, mutagen, carcinogen, reproductive toxicity, systemic target organ toxicity, aspiration hazard
Acute toxicity, Very toxic (fatal), Toxic etc
Harmful skin irritation, serious eye irritation
Harmful to the Environment
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Flammable gasses, liquids, solids, aerosols, organic peroxides, self-reactive, pyrophoric, self-heating etc
Explosive, self reactive, organic peroxide
oxidising gases, liquids, solids
Gasses under pressure


	First Aid Requirements 

Details to be found on the Material Safety Data Sheet

	Exposure Via
	First Aid Treatment

	Inhalation
	Move away the source generating dust or bring the victim away from the source of dust and place the victim outside to breathe fresh air. Consult a doctor without delay.

	Ingestion
	Rinse mouth with clean water. Drink water abundantly.

Do not induce vomiting. Call a doctor as soon as possible.

	Skin Contact
	Gently and carefully brush off all traces of the substance on the affected areas.

Abundantly wash with clean running water the affected area.

Take off contaminated clothing. If necessary seek medical advice.

	Eye Contact
	Wash eyes immediately with clean water or, if possible, with an isotonic liquid. Obtain medical advice.

	General advice
	No delayed effects known. Consult a doctor/phisician in all case of severe exposure to the substance or in case of doubt.
NHL lime does not have acute toxicity in respect of oral, skin or respiratory exposure. The substance is classified as irritant for the skin and respiratory ways and presents a risk of serious eyes damage. No deadly effects are suspected; the principal danger is restricted to localised effects (effect pH).

	The effects of the substance on the body.

Take into account any changes in the substances state, during the task

	Substance (s) Used In Task

(List below)
	Nature of Hazard(s) Associated with Substance

Detail the effect of the substance on the body throughout the duration of its use and changing states.

	Saint Astier (NHL)3.5
	Causes skin irritation

	Saint Astier (NHL)3.5
	Causes serious eye damage

	Saint Astier (NHL)3.5
	May cause respiratory irritation


Source, Duration and Risk of Exposure

	Identify at what stage of the task the exposure will happen and how. E.g. Inhalation of Rock wool fibres whilst opening bag.  

	Substance(s)


	Source(s) of Exposure

(include route of entry)
	Duration of Exposure

(Min / Hrs)
	Risk from Exposure

(High, Med, Low)

	Saint Astier (NHL)3.5
	Inhalation, eye and skin contact when handling bags for storage
	
	

	Saint Astier (NHL)3.5
	Inhalation, eye and skin contact when mixing
	
	

	Saint Astier (NHL)3.5
	Eye and skin contact when applying 
	
	

	Saint Astier (NHL)3.5
	Inhalation, eye and skin contact when containing spill
	
	

	Emergency and Disposal

Detail the requirements to deal with accidental release and disposal of the substance.

	Accidental release
	Ensure adequate ventilation, Avoid release of dust as much as possible. Keep away persons not wearing appropriate protective equipment.  Avoid all contact with skin, eyes and clothing. Wear appropriate protective equipment. Avoid inhaling dust

Ensure adequate ventilation or wear respiration masks Wear appropriate protective clothing

	Disposal
	Dispose of bags content/empty bags at a point of refuse collection. Before disposal, NHL lime should be made inert by wetting it to induce hardening and bags should be completely emptied.

	Fire Fighting
	The product is not combustible. Use all methods appropriate to the source of the fire.

	Control Measures

Identify actions to eliminate the hazard, substitute the hazardous for the less harmful, engineering control, competency or specific PPE required.

	Control Measure(s) required to work safely
	Completed

	Keep out of reach of children
	

	Store in a dry place.   Keep product dry if possible
	

	NHLs produce an exothermic reaction in contact with acids to form salts.

In presence of humidity the NHLs react with aluminium and brass producing hydrogen Ca(OH)2 + 2Al + 6H2O --> Ca[Al(OH)4]2 + 3 H2
	

	Dispose of bags content/empty bags at a point of refuse collection. Before disposal, NHL lime should be made inert by wetting it to induce hardening and bags should be completely emptied.
	

	Label all recipients where dust has been collected
	

	Wear protective gloves/clothing/eye and face protection
	

	Appropriate barrier creams can be used.
	

	Wash hands after each manipulation.
	

	General measures of hygiene at work are essential to ensure safe handling of the product. These include: Good personal practices, regular cleaning of the place of work, no alcohol drinking, eating or smoking at the place of work.
	

	Shower and change clothing at the end of work.
	

	Separate work clothing from other clothing. Clean them separately. Do not bring home any contaminated clothing.
	

	
	

	Authorised by The Responsible Manager
	Name:
	Signed:


	Dated:
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