Transport & Traffic Statement Planning Ref PLA-2026-000393
Site Location: 23 Dolphin Street, Ardwick, Manchester
Proposed Development: Commercial Office Space (Capacity: 30 Employees)

1. Trip Generation & Traffic Impact
· Peak Period Volume: An office of 30 people will generate an estimated 12 to 18 vehicle movements per day. The majority of these will take place during morning (08:00–09:00) and evening (17:00–18:00) peak hours.
· Network Capacity: This nominal volume represents less than one additional vehicle every 3–5 minutes during peak hours. It will cause zero noticeable impact or delay on the local highway network along Dolphin Street or the surrounding Ardwick road network.

2. Rear Yard Configuration & Parking Strategy
· Sustainable Parking Cap: In line with Manchester City Council's active transport and parking restrictions, private car parking will be strictly capped to prevent local congestion. The large rear yard will comfortably accommodate a maximum of 4 to 6 allocated staff/visitor vehicle bays.
· EV Charging: At least 20% of the yard's parking bays will feature active Electric Vehicle (EV) charging points, ensuring alignment with local climate action policies.
· On-Street Protection: Restricting on-site parking prevents workers from spilling over onto Dolphin Street, keeping local residential corridors completely clear.

3. Cycle Provisions (Utilising the Yard)
· Secure Bike Storage: To meet Greater Manchester's active travel targets, a portion of the large rear yard will be dedicated to a secure, covered, and illuminated Sheffield-stand cycle shelter. [1]
· Capacity: This shelter will accommodate a minimum of 4 to 6 bicycles (exceeding the standard 10–15% employee modal share ratio) to actively encourage sustainable commuting.
· End-of-Trip Infrastructure: The internal building layout will feature dedicated shower and changing facilities for staff.

4. Deliveries, Servicing, and Waste Management
· Off-Street Servicing: All delivery vans (DHL, Amazon, office suppliers) and refuse collection vehicles will utilize the large rear yard for loading and unloading. This takes 100% of servicing traffic off Dolphin Street.
· Turning Circle Safety: The yard provides sufficient clearance for a standard 3.5-tonne delivery van or an 11.2-meter refuse truck to perform a multi-point turn. This guarantees all vehicles can enter and exit the site in a forward gear, preventing hazardous reversing manoeuvres onto the public highway.

5. Accessibility & Public Transport Linkages
· Bus and Rail Proximity: The statement emphasizes that the majority of the 30 employees will travel sustainably. The site sits within a 5-minute walk of high-frequency bus corridors on the A6 Stockport Road and is highly accessible via Manchester Piccadilly Station and Ardwick Station.
· 6     Car sharing will be actively encouraged to fulfil the targets above. Showers and changing rooms are Provided to enable cyclists to be able to cycle to work and shower and change Onsite.


